# Trace events for debugging and performance instrumentation
#
# This file is processed by the tracetool script during the build.
#
# To add a new trace event:
#
# 1. Choose a name for the trace event.  Declare its arguments and format
#    string.
#
# 2. Call the trace event from code using trace_##name, e.g. multiwrite_cb() ->
#    trace_multiwrite_cb().  The source file must #include "trace.h".
#
# Format of a trace event:
#
# [disable] <name>(<type1> <arg1>[, <type2> <arg2>] ...) "<format-string>"
#
# Example: g_malloc(size_t size) "size %zu"
#
# The "disable" keyword will build without the trace event.
#
# The <name> must be a valid as a C function name.
#
# Types should be standard C types.  Use void * for pointers because the trace
# system may not have the necessary headers included.
#
# The <format-string> should be a sprintf()-compatible format string.

# util/oslib-win32.c
# util/oslib-posix.c
qemu_memalign(size_t alignment, size_t size, void *ptr) "alignment %zu size %zu ptr %p"
qemu_anon_ram_alloc(size_t size, void *ptr) "size %zu ptr %p"
qemu_vfree(void *ptr) "ptr %p"
qemu_anon_ram_free(void *ptr, size_t size) "ptr %p size %zu"

# hw/virtio/virtio.c
virtqueue_fill(void *vq, const void *elem, unsigned int len, unsigned int idx) "vq %p elem %p len %u idx %u"
virtqueue_flush(void *vq, unsigned int count) "vq %p count %u"
virtqueue_pop(void *vq, void *elem, unsigned int in_num, unsigned int out_num) "vq %p elem %p in_num %u out_num %u"
virtio_queue_notify(void *vdev, int n, void *vq) "vdev %p n %d vq %p"
virtio_irq(void *vq) "vq %p"
virtio_notify(void *vdev, void *vq) "vdev %p vq %p"
virtio_set_status(void *vdev, uint8_t val) "vdev %p val %u"

# hw/virtio/virtio-rng.c
virtio_rng_guest_not_ready(void *rng) "rng %p: guest not ready"
virtio_rng_pushed(void *rng, size_t len) "rng %p: %zd bytes pushed"
virtio_rng_request(void *rng, size_t size, unsigned quota) "rng %p: %zd bytes requested, %u bytes quota left"

# hw/char/virtio-serial-bus.c
virtio_serial_send_control_event(unsigned int port, uint16_t event, uint16_t value) "port %u, event %u, value %u"
virtio_serial_throttle_port(unsigned int port, bool throttle) "port %u, throttle %d"
virtio_serial_handle_control_message(uint16_t event, uint16_t value) "event %u, value %u"
virtio_serial_handle_control_message_port(unsigned int port) "port %u"

# hw/char/virtio-console.c
virtio_console_flush_buf(unsigned int port, size_t len, ssize_t ret) "port %u, in_len %zu, out_len %zd"
virtio_console_chr_read(unsigned int port, int size) "port %u, size %d"
virtio_console_chr_event(unsigned int port, int event) "port %u, event %d"

# block.c
bdrv_open_common(void *bs, const char *filename, int flags, const char *format_name) "bs %p filename \"%s\" flags %#x format_name \"%s\""
multiwrite_cb(void *mcb, int ret) "mcb %p ret %d"
bdrv_aio_multiwrite(void *mcb, int num_callbacks, int num_reqs) "mcb %p num_callbacks %d num_reqs %d"
bdrv_aio_discard(void *bs, int64_t sector_num, int nb_sectors, void *opaque) "bs %p sector_num %"PRId64" nb_sectors %d opaque %p"
bdrv_aio_flush(void *bs, void *opaque) "bs %p opaque %p"
bdrv_aio_readv(void *bs, int64_t sector_num, int nb_sectors, void *opaque) "bs %p sector_num %"PRId64" nb_sectors %d opaque %p"
bdrv_aio_writev(void *bs, int64_t sector_num, int nb_sectors, void *opaque) "bs %p sector_num %"PRId64" nb_sectors %d opaque %p"
bdrv_aio_write_zeroes(void *bs, int64_t sector_num, int nb_sectors, int flags, void *opaque) "bs %p sector_num %"PRId64" nb_sectors %d flags %#x opaque %p"
bdrv_lock_medium(void *bs, bool locked) "bs %p locked %d"
bdrv_co_readv(void *bs, int64_t sector_num, int nb_sector) "bs %p sector_num %"PRId64" nb_sectors %d"
bdrv_co_copy_on_readv(void *bs, int64_t sector_num, int nb_sector) "bs %p sector_num %"PRId64" nb_sectors %d"
bdrv_co_writev(void *bs, int64_t sector_num, int nb_sector) "bs %p sector_num %"PRId64" nb_sectors %d"
bdrv_co_write_zeroes(void *bs, int64_t sector_num, int nb_sector, int flags) "bs %p sector_num %"PRId64" nb_sectors %d flags %#x"
bdrv_co_io_em(void *bs, int64_t sector_num, int nb_sectors, int is_write, void *acb) "bs %p sector_num %"PRId64" nb_sectors %d is_write %d acb %p"
bdrv_co_do_copy_on_readv(void *bs, int64_t sector_num, int nb_sectors, int64_t cluster_sector_num, int cluster_nb_sectors) "bs %p sector_num %"PRId64" nb_sectors %d cluster_sector_num %"PRId64" cluster_nb_sectors %d"

# block/stream.c
stream_one_iteration(void *s, int64_t sector_num, int nb_sectors, int is_allocated) "s %p sector_num %"PRId64" nb_sectors %d is_allocated %d"
stream_start(void *bs, void *base, void *s, void *co, void *opaque) "bs %p base %p s %p co %p opaque %p"

# block/commit.c
commit_one_iteration(void *s, int64_t sector_num, int nb_sectors, int is_allocated) "s %p sector_num %"PRId64" nb_sectors %d is_allocated %d"
commit_start(void *bs, void *base, void *top, void *s, void *co, void *opaque) "bs %p base %p top %p s %p co %p opaque %p"

# block/mirror.c
mirror_start(void *bs, void *s, void *co, void *opaque) "bs %p s %p co %p opaque %p"
mirror_restart_iter(void *s, int64_t cnt) "s %p dirty count %"PRId64
mirror_before_flush(void *s) "s %p"
mirror_before_drain(void *s, int64_t cnt) "s %p dirty count %"PRId64
mirror_before_sleep(void *s, int64_t cnt, int synced, uint64_t delay_ns) "s %p dirty count %"PRId64" synced %d delay %"PRIu64"ns"
mirror_one_iteration(void *s, int64_t sector_num, int nb_sectors) "s %p sector_num %"PRId64" nb_sectors %d"
mirror_iteration_done(void *s, int64_t sector_num, int nb_sectors, int ret) "s %p sector_num %"PRId64" nb_sectors %d ret %d"
mirror_yield(void *s, int64_t cnt, int buf_free_count, int in_flight) "s %p dirty count %"PRId64" free buffers %d in_flight %d"
mirror_yield_in_flight(void *s, int64_t sector_num, int in_flight) "s %p sector_num %"PRId64" in_flight %d"
mirror_yield_buf_busy(void *s, int nb_chunks, int in_flight) "s %p requested chunks %d in_flight %d"
mirror_break_buf_busy(void *s, int nb_chunks, int in_flight) "s %p requested chunks %d in_flight %d"

# block/backup.c
backup_do_cow_enter(void *job, int64_t start, int64_t sector_num, int nb_sectors) "job %p start %"PRId64" sector_num %"PRId64" nb_sectors %d"
backup_do_cow_return(void *job, int64_t sector_num, int nb_sectors, int ret) "job %p sector_num %"PRId64" nb_sectors %d ret %d"
backup_do_cow_skip(void *job, int64_t start) "job %p start %"PRId64
backup_do_cow_process(void *job, int64_t start) "job %p start %"PRId64
backup_do_cow_read_fail(void *job, int64_t start, int ret) "job %p start %"PRId64" ret %d"
backup_do_cow_write_fail(void *job, int64_t start, int ret) "job %p start %"PRId64" ret %d"

# blockdev.c
qmp_block_job_cancel(void *job) "job %p"
qmp_block_job_pause(void *job) "job %p"
qmp_block_job_resume(void *job) "job %p"
qmp_block_job_complete(void *job) "job %p"
block_job_cb(void *bs, void *job, int ret) "bs %p job %p ret %d"
qmp_block_stream(void *bs, void *job) "bs %p job %p"

# hw/block/virtio-blk.c
virtio_blk_req_complete(void *req, int status) "req %p status %d"
virtio_blk_rw_complete(void *req, int ret) "req %p ret %d"
virtio_blk_handle_write(void *req, uint64_t sector, size_t nsectors) "req %p sector %"PRIu64" nsectors %zu"
virtio_blk_handle_read(void *req, uint64_t sector, size_t nsectors) "req %p sector %"PRIu64" nsectors %zu"
virtio_blk_submit_multireq(void *mrb, int start, int num_reqs, uint64_t sector, size_t nsectors, bool is_write) "mrb %p start %d num_reqs %d sector %"PRIu64" nsectors %zu is_write %d"

# hw/block/dataplane/virtio-blk.c
virtio_blk_data_plane_start(void *s) "dataplane %p"
virtio_blk_data_plane_stop(void *s) "dataplane %p"
virtio_blk_data_plane_process_request(void *s, unsigned int out_num, unsigned int in_num, unsigned int head) "dataplane %p out_num %u in_num %u head %u"

# hw/virtio/dataplane/vring.c
vring_setup(uint64_t physical, void *desc, void *avail, void *used) "vring physical %#"PRIx64" desc %p avail %p used %p"

# thread-pool.c
thread_pool_submit(void *pool, void *req, void *opaque) "pool %p req %p opaque %p"
thread_pool_complete(void *pool, void *req, void *opaque, int ret) "pool %p req %p opaque %p ret %d"
thread_pool_cancel(void *req, void *opaque) "req %p opaque %p"

# block/raw-win32.c
# block/raw-posix.c
paio_submit_co(int64_t sector_num, int nb_sectors, int type) "sector_num %"PRId64" nb_sectors %d type %d"
paio_submit(void *acb, void *opaque, int64_t sector_num, int nb_sectors, int type) "acb %p opaque %p sector_num %"PRId64" nb_sectors %d type %d"

# ioport.c
cpu_in(unsigned int addr, unsigned int val) "addr %#x value %u"
cpu_out(unsigned int addr, unsigned int val) "addr %#x value %u"

# balloon.c
# Since requests are raised via monitor, not many tracepoints are needed.
balloon_event(void *opaque, unsigned long addr) "opaque %p addr %lu"
virtio_balloon_handle_output(const char *name, uint64_t gpa) "setion name: %s gpa: %"PRIx64""
virtio_balloon_get_config(uint32_t num_pages, uint32_t acutal) "num_pages: %d acutal: %d"
virtio_balloon_set_config(uint32_t acutal, uint32_t oldacutal) "acutal: %d oldacutal: %d"
virtio_balloon_to_target(uint64_t target, uint32_t num_pages) "balloon target: %"PRIx64" num_pages: %d"

# hw/intc/apic_common.c
cpu_set_apic_base(uint64_t val) "%016"PRIx64
cpu_get_apic_base(uint64_t val) "%016"PRIx64
# coalescing
apic_report_irq_delivered(int apic_irq_delivered) "coalescing %d"
apic_reset_irq_delivered(int apic_irq_delivered) "old coalescing %d"
apic_get_irq_delivered(int apic_irq_delivered) "returning coalescing %d"

# hw/intc/apic.c
apic_local_deliver(int vector, uint32_t lvt) "vector %d delivery mode %d"
apic_deliver_irq(uint8_t dest, uint8_t dest_mode, uint8_t delivery_mode, uint8_t vector_num, uint8_t trigger_mode) "dest %d dest_mode %d delivery_mode %d vector %d trigger_mode %d"
apic_mem_readl(uint64_t addr, uint32_t val)  "%"PRIx64" = %08x"
apic_mem_writel(uint64_t addr, uint32_t val) "%"PRIx64" = %08x"

# hw/audio/cs4231.c
cs4231_mem_readl_dreg(uint32_t reg, uint32_t ret) "read dreg %d: 0x%02x"
cs4231_mem_readl_reg(uint32_t reg, uint32_t ret) "read reg %d: 0x%08x"
cs4231_mem_writel_reg(uint32_t reg, uint32_t old, uint32_t val) "write reg %d: 0x%08x -> 0x%08x"
cs4231_mem_writel_dreg(uint32_t reg, uint32_t old, uint32_t val) "write dreg %d: 0x%02x -> 0x%02x"

# hw/nvram/ds1225y.c
nvram_read(uint32_t addr, uint32_t ret) "read addr %d: 0x%02x"
nvram_write(uint32_t addr, uint32_t old, uint32_t val) "write addr %d: 0x%02x -> 0x%02x"

# hw/misc/eccmemctl.c
ecc_mem_writel_mer(uint32_t val) "Write memory enable %08x"
ecc_mem_writel_mdr(uint32_t val) "Write memory delay %08x"
ecc_mem_writel_mfsr(uint32_t val) "Write memory fault status %08x"
ecc_mem_writel_vcr(uint32_t val) "Write slot configuration %08x"
ecc_mem_writel_dr(uint32_t val) "Write diagnostic %08x"
ecc_mem_writel_ecr0(uint32_t val) "Write event count 1 %08x"
ecc_mem_writel_ecr1(uint32_t val) "Write event count 2 %08x"
ecc_mem_readl_mer(uint32_t ret) "Read memory enable %08x"
ecc_mem_readl_mdr(uint32_t ret) "Read memory delay %08x"
ecc_mem_readl_mfsr(uint32_t ret) "Read memory fault status %08x"
ecc_mem_readl_vcr(uint32_t ret) "Read slot configuration %08x"
ecc_mem_readl_mfar0(uint32_t ret) "Read memory fault address 0 %08x"
ecc_mem_readl_mfar1(uint32_t ret) "Read memory fault address 1 %08x"
ecc_mem_readl_dr(uint32_t ret) "Read diagnostic %08x"
ecc_mem_readl_ecr0(uint32_t ret) "Read event count 1 %08x"
ecc_mem_readl_ecr1(uint32_t ret) "Read event count 2 %08x"
ecc_diag_mem_writeb(uint64_t addr, uint32_t val) "Write diagnostic %"PRId64" = %02x"
ecc_diag_mem_readb(uint64_t addr, uint32_t ret) "Read diagnostic %"PRId64"= %02x"

# hw/nvram/fw_cfg.c
fw_cfg_select(void *s, uint16_t key, int ret) "%p key %d = %d"
fw_cfg_read(void *s, uint8_t ret) "%p = %d"
fw_cfg_add_file(void *s, int index, char *name, size_t len) "%p #%d: %s (%zd bytes)"

# hw/block/hd-geometry.c
hd_geometry_lchs_guess(void *blk, int cyls, int heads, int secs) "blk %p LCHS %d %d %d"
hd_geometry_guess(void *blk, uint32_t cyls, uint32_t heads, uint32_t secs, int trans) "blk %p CHS %u %u %u trans %d"

# hw/display/jazz_led.c
jazz_led_read(uint64_t addr, uint8_t val) "read addr=0x%"PRIx64": 0x%x"
jazz_led_write(uint64_t addr, uint8_t new) "write addr=0x%"PRIx64": 0x%x"

# hw/display/xenfb.c
xenfb_mouse_event(void *opaque, int dx, int dy, int dz, int button_state, int abs_pointer_wanted) "%p x %d y %d z %d bs %#x abs %d"
xenfb_input_connected(void *xendev, int abs_pointer_wanted) "%p abs %d"

# hw/net/lance.c
lance_mem_readw(uint64_t addr, uint32_t ret) "addr=%"PRIx64"val=0x%04x"
lance_mem_writew(uint64_t addr, uint32_t val) "addr=%"PRIx64"val=0x%04x"

# hw/intc/slavio_intctl.c
slavio_intctl_mem_readl(uint32_t cpu, uint64_t addr, uint32_t ret) "read cpu %d reg 0x%"PRIx64" = %x"
slavio_intctl_mem_writel(uint32_t cpu, uint64_t addr, uint32_t val) "write cpu %d reg 0x%"PRIx64" = %x"
slavio_intctl_mem_writel_clear(uint32_t cpu, uint32_t val, uint32_t intreg_pending) "Cleared cpu %d irq mask %x, curmask %x"
slavio_intctl_mem_writel_set(uint32_t cpu, uint32_t val, uint32_t intreg_pending) "Set cpu %d irq mask %x, curmask %x"
slavio_intctlm_mem_readl(uint64_t addr, uint32_t ret) "read system reg 0x%"PRIx64" = %x"
slavio_intctlm_mem_writel(uint64_t addr, uint32_t val) "write system reg 0x%"PRIx64" = %x"
slavio_intctlm_mem_writel_enable(uint32_t val, uint32_t intregm_disabled) "Enabled master irq mask %x, curmask %x"
slavio_intctlm_mem_writel_disable(uint32_t val, uint32_t intregm_disabled) "Disabled master irq mask %x, curmask %x"
slavio_intctlm_mem_writel_target(uint32_t cpu) "Set master irq cpu %d"
slavio_check_interrupts(uint32_t pending, uint32_t intregm_disabled) "pending %x disabled %x"
slavio_set_irq(uint32_t target_cpu, int irq, uint32_t pil, int level) "Set cpu %d irq %d -> pil %d level %d"
slavio_set_timer_irq_cpu(int cpu, int level) "Set cpu %d local timer level %d"

# hw/input/ps2.c
ps2_put_keycode(void *opaque, int keycode) "%p keycode %d"
ps2_read_data(void *opaque) "%p"
ps2_set_ledstate(void *s, int ledstate) "%p ledstate %d"
ps2_reset_keyboard(void *s) "%p"
ps2_write_keyboard(void *opaque, int val) "%p val %d"
ps2_keyboard_set_translation(void *opaque, int mode) "%p mode %d"
ps2_mouse_send_packet(void *s, int dx1, int dy1, int dz1, int b) "%p x %d y %d z %d bs %#x"
ps2_mouse_event_disabled(void *opaque, int dx, int dy, int dz, int buttons_state, int mouse_dx, int mouse_dy, int mouse_dz) "%p x %d y %d z %d bs %#x mx %d my %d mz %d "
ps2_mouse_event(void *opaque, int dx, int dy, int dz, int buttons_state, int mouse_dx, int mouse_dy, int mouse_dz) "%p x %d y %d z %d bs %#x mx %d my %d mz %d "
ps2_mouse_fake_event(void *opaque) "%p"
ps2_write_mouse(void *opaque, int val) "%p val %d"
ps2_kbd_reset(void *opaque) "%p"
ps2_mouse_reset(void *opaque) "%p"
ps2_kbd_init(void *s) "%p"
ps2_mouse_init(void *s) "%p"

# hw/misc/slavio_misc.c
slavio_misc_update_irq_raise(void) "Raise IRQ"
slavio_misc_update_irq_lower(void) "Lower IRQ"
slavio_set_power_fail(int power_failing, uint8_t config) "Power fail: %d, config: %d"
slavio_cfg_mem_writeb(uint32_t val) "Write config %02x"
slavio_cfg_mem_readb(uint32_t ret) "Read config %02x"
slavio_diag_mem_writeb(uint32_t val) "Write diag %02x"
slavio_diag_mem_readb(uint32_t ret) "Read diag %02x"
slavio_mdm_mem_writeb(uint32_t val) "Write modem control %02x"
slavio_mdm_mem_readb(uint32_t ret) "Read modem control %02x"
slavio_aux1_mem_writeb(uint32_t val) "Write aux1 %02x"
slavio_aux1_mem_readb(uint32_t ret) "Read aux1 %02x"
slavio_aux2_mem_writeb(uint32_t val) "Write aux2 %02x"
slavio_aux2_mem_readb(uint32_t ret) "Read aux2 %02x"
apc_mem_writeb(uint32_t val) "Write power management %02x"
apc_mem_readb(uint32_t ret) "Read power management %02x"
slavio_sysctrl_mem_writel(uint32_t val) "Write system control %08x"
slavio_sysctrl_mem_readl(uint32_t ret) "Read system control %08x"
slavio_led_mem_writew(uint32_t val) "Write diagnostic LED %04x"
slavio_led_mem_readw(uint32_t ret) "Read diagnostic LED %04x"

# hw/timer/slavio_timer.c
slavio_timer_get_out(uint64_t limit, uint32_t counthigh, uint32_t count) "limit %"PRIx64" count %x%08x"
slavio_timer_irq(uint32_t counthigh, uint32_t count) "callback: count %x%08x"
slavio_timer_mem_readl_invalid(uint64_t addr) "invalid read address %"PRIx64
slavio_timer_mem_readl(uint64_t addr, uint32_t ret) "read %"PRIx64" = %08x"
slavio_timer_mem_writel(uint64_t addr, uint32_t val) "write %"PRIx64" = %08x"
slavio_timer_mem_writel_limit(unsigned int timer_index, uint64_t count) "processor %d user timer set to %016"PRIx64
slavio_timer_mem_writel_counter_invalid(void) "not user timer"
slavio_timer_mem_writel_status_start(unsigned int timer_index) "processor %d user timer started"
slavio_timer_mem_writel_status_stop(unsigned int timer_index) "processor %d user timer stopped"
slavio_timer_mem_writel_mode_user(unsigned int timer_index) "processor %d changed from counter to user timer"
slavio_timer_mem_writel_mode_counter(unsigned int timer_index) "processor %d changed from user timer to counter"
slavio_timer_mem_writel_mode_invalid(void) "not system timer"
slavio_timer_mem_writel_invalid(uint64_t addr) "invalid write address %"PRIx64

# hw/dma/rc4030.c
jazzio_read(uint64_t addr, uint32_t ret) "read reg[0x%"PRIx64"] = 0x%x"
jazzio_write(uint64_t addr, uint32_t val) "write reg[0x%"PRIx64"] = 0x%x"
rc4030_read(uint64_t addr, uint32_t ret) "read reg[0x%"PRIx64"] = 0x%x"
rc4030_write(uint64_t addr, uint32_t val) "write reg[0x%"PRIx64"] = 0x%x"

# hw/dma/sparc32_dma.c
ledma_memory_read(uint64_t addr) "DMA read addr 0x%"PRIx64
ledma_memory_write(uint64_t addr) "DMA write addr 0x%"PRIx64
sparc32_dma_set_irq_raise(void) "Raise IRQ"
sparc32_dma_set_irq_lower(void) "Lower IRQ"
espdma_memory_read(uint32_t addr) "DMA read addr 0x%08x"
espdma_memory_write(uint32_t addr) "DMA write addr 0x%08x"
sparc32_dma_mem_readl(uint64_t addr, uint32_t ret) "read dmareg %"PRIx64": 0x%08x"
sparc32_dma_mem_writel(uint64_t addr, uint32_t old, uint32_t val) "write dmareg %"PRIx64": 0x%08x -> 0x%08x"
sparc32_dma_enable_raise(void) "Raise DMA enable"
sparc32_dma_enable_lower(void) "Lower DMA enable"

# hw/sparc/sun4m.c
sun4m_cpu_interrupt(unsigned int level) "Set CPU IRQ %d"
sun4m_cpu_reset_interrupt(unsigned int level) "Reset CPU IRQ %d"
sun4m_cpu_set_irq_raise(int level) "Raise CPU IRQ %d"
sun4m_cpu_set_irq_lower(int level) "Lower CPU IRQ %d"

# hw/dma/sun4m_iommu.c
sun4m_iommu_mem_readl(uint64_t addr, uint32_t ret) "read reg[%"PRIx64"] = %x"
sun4m_iommu_mem_writel(uint64_t addr, uint32_t val) "write reg[%"PRIx64"] = %x"
sun4m_iommu_mem_writel_ctrl(uint64_t iostart) "iostart = %"PRIx64
sun4m_iommu_mem_writel_tlbflush(uint32_t val) "tlb flush %x"
sun4m_iommu_mem_writel_pgflush(uint32_t val) "page flush %x"
sun4m_iommu_page_get_flags(uint64_t pa, uint64_t iopte, uint32_t ret) "get flags addr %"PRIx64" => pte %"PRIx64", *pte = %x"
sun4m_iommu_translate_pa(uint64_t addr, uint64_t pa, uint32_t iopte) "xlate dva %"PRIx64" => pa %"PRIx64" iopte = %x"
sun4m_iommu_bad_addr(uint64_t addr) "bad addr %"PRIx64

# hw/usb/core.c
usb_packet_state_change(int bus, const char *port, int ep, void *p, const char *o, const char *n) "bus %d, port %s, ep %d, packet %p, state %s -> %s"
usb_packet_state_fault(int bus, const char *port, int ep, void *p, const char *o, const char *n) "bus %d, port %s, ep %d, packet %p, state %s, expected %s"

# hw/usb/bus.c
usb_port_claim(int bus, const char *port) "bus %d, port %s"
usb_port_attach(int bus, const char *port, const char *devspeed, const char *portspeed) "bus %d, port %s, devspeed %s, portspeed %s"
usb_port_detach(int bus, const char *port) "bus %d, port %s"
usb_port_release(int bus, const char *port) "bus %d, port %s"

# hw/usb/hcd-ohci.c
usb_ohci_iso_td_read_failed(uint32_t addr) "ISO_TD read error at %x"
usb_ohci_iso_td_head(uint32_t head, uint32_t tail, uint32_t flags, uint32_t bp, uint32_t next, uint32_t be, uint32_t framenum, uint32_t startframe, uint32_t framecount, int rel_frame_num) "ISO_TD ED head 0x%.8x tailp 0x%.8x\n0x%.8x 0x%.8x 0x%.8x 0x%.8x\nframe_number 0x%.8x starting_frame 0x%.8x\nframe_count  0x%.8x relative %d"
usb_ohci_iso_td_head_offset(uint32_t o0, uint32_t o1, uint32_t o2, uint32_t o3, uint32_t o4, uint32_t o5, uint32_t o6, uint32_t o7) "0x%.8x 0x%.8x 0x%.8x 0x%.8x 0x%.8x 0x%.8x 0x%.8x 0x%.8x"
usb_ohci_iso_td_relative_frame_number_neg(int rel) "ISO_TD R=%d < 0"
usb_ohci_iso_td_relative_frame_number_big(int rel, int count) "ISO_TD R=%d > FC=%d"
usb_ohci_iso_td_bad_direction(int dir) "Bad direction %d"
usb_ohci_iso_td_bad_bp_be(uint32_t bp, uint32_t be) "ISO_TD bp 0x%.8x be 0x%.8x"
usb_ohci_iso_td_bad_cc_not_accessed(uint32_t start, uint32_t next) "ISO_TD cc != not accessed 0x%.8x 0x%.8x"
usb_ohci_iso_td_bad_cc_overrun(uint32_t start, uint32_t next) "ISO_TD start_offset=0x%.8x > next_offset=0x%.8x"
usb_ohci_iso_td_so(uint32_t so, uint32_t eo, uint32_t s, uint32_t e, const char *str, ssize_t len, int ret) "0x%.8x eo 0x%.8x\nsa 0x%.8x ea 0x%.8x\ndir %s len %zu ret %d"
usb_ohci_iso_td_data_overrun(int ret, ssize_t len) "DataOverrun %d > %zu"
usb_ohci_iso_td_data_underrun(int ret) "DataUnderrun %d"
usb_ohci_iso_td_nak(int ret) "got NAK/STALL %d"
usb_ohci_iso_td_bad_response(int ret) "Bad device response %d"
usb_ohci_port_attach(int index) "port #%d"
usb_ohci_port_detach(int index) "port #%d"
usb_ohci_port_wakeup(int index) "port #%d"
usb_ohci_port_suspend(int index) "port #%d"
usb_ohci_port_reset(int index) "port #%d"
usb_ohci_remote_wakeup(const char *s) "%s: SUSPEND->RESUME"
usb_ohci_reset(const char *s) "%s"
usb_ohci_start(const char *s) "%s: USB Operational"
usb_ohci_resume(const char *s) "%s: USB Resume"
usb_ohci_stop(const char *s) "%s: USB Suspended"
usb_ohci_exit(const char *s) "%s"
usb_ohci_set_ctl(const char *s, uint32_t new_state) "%s: new state 0x%x"
usb_ohci_td_underrun(void) ""
usb_ohci_td_dev_error(void) ""
usb_ohci_td_nak(void) ""
usb_ohci_td_stall(void) ""
usb_ohci_td_babble(void) ""
usb_ohci_td_bad_device_response(int rc) "%d"
usb_ohci_td_read_error(uint32_t addr) "TD read error at %x"
usb_ohci_td_bad_direction(int dir) "Bad direction %d"
usb_ohci_td_skip_async(void) ""
usb_ohci_td_pkt_hdr(uint32_t addr, int64_t pktlen, int64_t len, const char *s, int flag_r, uint32_t cbp, uint32_t be) " TD @ 0x%.8x %" PRId64 " of %" PRId64 " bytes %s r=%d cbp=0x%.8x be=0x%.8x"
usb_ohci_td_pkt_short(const char *dir, const char *buf) "%s data: %s"
usb_ohci_td_pkt_full(const char *dir, const char *buf) "%s data: %s"
usb_ohci_td_too_many_pending(void) ""
usb_ohci_td_packet_status(int status) "status=%d"
usb_ohci_ed_read_error(uint32_t addr) "ED read error at %x"
usb_ohci_ed_pkt(uint32_t cur, int h, int c, uint32_t head, uint32_t tail, uint32_t next) "ED @ 0x%.8x h=%u c=%u\n  head=0x%.8x tailp=0x%.8x next=0x%.8x"
usb_ohci_ed_pkt_flags(uint32_t fa, uint32_t en, uint32_t d, int s, int k, int f, uint32_t mps) "fa=%u en=%u d=%u s=%u k=%u f=%u mps=%u"
usb_ohci_hcca_read_error(uint32_t addr) "HCCA read error at %x"
usb_ohci_mem_read_unaligned(uint32_t addr) "at %x"
usb_ohci_mem_read_bad_offset(uint32_t addr) "%x"
usb_ohci_mem_write_unaligned(uint32_t addr) "at %x"
usb_ohci_mem_write_bad_offset(uint32_t addr) "%x"
usb_ohci_process_lists(uint32_t head, uint32_t cur) "head %x, cur %x"
usb_ohci_bus_eof_timer_failed(const char *name) "%s: timer_new_ns failed"
usb_ohci_set_frame_interval(const char *name, uint16_t fi_x, uint16_t fi_u) "%s: FrameInterval = 0x%x (%u)"
usb_ohci_hub_power_up(void) "powered up all ports"
usb_ohci_hub_power_down(void) "powered down all ports"
usb_ohci_init_time(int64_t frametime, int64_t bittime) "usb_bit_time=%" PRId64 " usb_frame_time=%" PRId64
usb_ohci_die(void) ""
usb_ohci_async_complete(void) ""

# hw/usb/hcd-ehci.c
usb_ehci_reset(void) "=== RESET ==="
usb_ehci_unrealize(void) "=== UNREALIZE ==="
usb_ehci_opreg_read(uint32_t addr, const char *str, uint32_t val) "rd mmio %04x [%s] = %x"
usb_ehci_opreg_write(uint32_t addr, const char *str, uint32_t val) "wr mmio %04x [%s] = %x"
usb_ehci_opreg_change(uint32_t addr, const char *str, uint32_t new, uint32_t old) "ch mmio %04x [%s] = %x (old: %x)"
usb_ehci_portsc_read(uint32_t addr, uint32_t port, uint32_t val) "rd mmio %04x [port %d] = %x"
usb_ehci_portsc_write(uint32_t addr, uint32_t port, uint32_t val) "wr mmio %04x [port %d] = %x"
usb_ehci_portsc_change(uint32_t addr, uint32_t port, uint32_t new, uint32_t old) "ch mmio %04x [port %d] = %x (old: %x)"
usb_ehci_usbsts(const char *sts, int state) "usbsts %s %d"
usb_ehci_state(const char *schedule, const char *state) "%s schedule %s"
usb_ehci_qh_ptrs(void *q, uint32_t addr, uint32_t nxt, uint32_t c_qtd, uint32_t n_qtd, uint32_t a_qtd) "q %p - QH @ %08x: next %08x qtds %08x,%08x,%08x"
usb_ehci_qh_fields(uint32_t addr, int rl, int mplen, int eps, int ep, int devaddr) "QH @ %08x - rl %d, mplen %d, eps %d, ep %d, dev %d"
usb_ehci_qh_bits(uint32_t addr, int c, int h, int dtc, int i) "QH @ %08x - c %d, h %d, dtc %d, i %d"
usb_ehci_qtd_ptrs(void *q, uint32_t addr, uint32_t nxt, uint32_t altnext) "q %p - QTD @ %08x: next %08x altnext %08x"
usb_ehci_qtd_fields(uint32_t addr, int tbytes, int cpage, int cerr, int pid) "QTD @ %08x - tbytes %d, cpage %d, cerr %d, pid %d"
usb_ehci_qtd_bits(uint32_t addr, int ioc, int active, int halt, int babble, int xacterr) "QTD @ %08x - ioc %d, active %d, halt %d, babble %d, xacterr %d"
usb_ehci_itd(uint32_t addr, uint32_t nxt, uint32_t mplen, uint32_t mult, uint32_t ep, uint32_t devaddr) "ITD @ %08x: next %08x - mplen %d, mult %d, ep %d, dev %d"
usb_ehci_sitd(uint32_t addr, uint32_t nxt, uint32_t active) "ITD @ %08x: next %08x - active %d"
usb_ehci_port_attach(uint32_t port, const char *owner, const char *device) "attach port #%d, owner %s, device %s"
usb_ehci_port_detach(uint32_t port, const char *owner) "detach port #%d, owner %s"
usb_ehci_port_reset(uint32_t port, int enable) "reset port #%d - %d"
usb_ehci_port_suspend(uint32_t port) "port #%d"
usb_ehci_port_wakeup(uint32_t port) "port #%d"
usb_ehci_port_resume(uint32_t port) "port #%d"
usb_ehci_queue_action(void *q, const char *action) "q %p: %s"
usb_ehci_packet_action(void *q, void *p, const char *action) "q %p p %p: %s"
usb_ehci_irq(uint32_t level, uint32_t frindex, uint32_t sts, uint32_t mask) "level %d, frindex 0x%04x, sts 0x%x, mask 0x%x"
usb_ehci_guest_bug(const char *reason) "%s"
usb_ehci_doorbell_ring(void) ""
usb_ehci_doorbell_ack(void) ""
usb_ehci_dma_error(void) ""

# hw/usb/hcd-uhci.c
usb_uhci_reset(void) "=== RESET ==="
usb_uhci_exit(void) "=== EXIT ==="
usb_uhci_schedule_start(void) ""
usb_uhci_schedule_stop(void) ""
usb_uhci_frame_start(uint32_t num) "nr %d"
usb_uhci_frame_stop_bandwidth(void) ""
usb_uhci_frame_loop_stop_idle(void) ""
usb_uhci_frame_loop_continue(void) ""
usb_uhci_mmio_readw(uint32_t addr, uint32_t val) "addr 0x%04x, ret 0x%04x"
usb_uhci_mmio_writew(uint32_t addr, uint32_t val) "addr 0x%04x, val 0x%04x"
usb_uhci_queue_add(uint32_t token) "token 0x%x"
usb_uhci_queue_del(uint32_t token, const char *reason) "token 0x%x: %s"
usb_uhci_packet_add(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_link_async(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_unlink_async(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_cancel(uint32_t token, uint32_t addr, int done) "token 0x%x, td 0x%x, done %d"
usb_uhci_packet_complete_success(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_complete_shortxfer(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_complete_stall(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_complete_babble(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_complete_error(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_packet_del(uint32_t token, uint32_t addr) "token 0x%x, td 0x%x"
usb_uhci_qh_load(uint32_t qh) "qh 0x%x"
usb_uhci_td_load(uint32_t qh, uint32_t td, uint32_t ctrl, uint32_t token) "qh 0x%x, td 0x%x, ctrl 0x%x, token 0x%x"
usb_uhci_td_queue(uint32_t td, uint32_t ctrl, uint32_t token) "td 0x%x, ctrl 0x%x, token 0x%x"
usb_uhci_td_nextqh(uint32_t qh, uint32_t td) "qh 0x%x, td 0x%x"
usb_uhci_td_async(uint32_t qh, uint32_t td) "qh 0x%x, td 0x%x"
usb_uhci_td_complete(uint32_t qh, uint32_t td) "qh 0x%x, td 0x%x"

# hw/usb/hcd-xhci.c
usb_xhci_reset(void) "=== RESET ==="
usb_xhci_exit(void) "=== EXIT ==="
usb_xhci_run(void) ""
usb_xhci_stop(void) ""
usb_xhci_cap_read(uint32_t off, uint32_t val) "off 0x%04x, ret 0x%08x"
usb_xhci_oper_read(uint32_t off, uint32_t val) "off 0x%04x, ret 0x%08x"
usb_xhci_port_read(uint32_t port, uint32_t off, uint32_t val) "port %d, off 0x%04x, ret 0x%08x"
usb_xhci_runtime_read(uint32_t off, uint32_t val) "off 0x%04x, ret 0x%08x"
usb_xhci_doorbell_read(uint32_t off, uint32_t val) "off 0x%04x, ret 0x%08x"
usb_xhci_oper_write(uint32_t off, uint32_t val) "off 0x%04x, val 0x%08x"
usb_xhci_port_write(uint32_t port, uint32_t off, uint32_t val) "port %d, off 0x%04x, val 0x%08x"
usb_xhci_runtime_write(uint32_t off, uint32_t val) "off 0x%04x, val 0x%08x"
usb_xhci_doorbell_write(uint32_t off, uint32_t val) "off 0x%04x, val 0x%08x"
usb_xhci_irq_intx(uint32_t level) "level %d"
usb_xhci_irq_msi(uint32_t nr) "nr %d"
usb_xhci_irq_msix(uint32_t nr) "nr %d"
usb_xhci_irq_msix_use(uint32_t nr) "nr %d"
usb_xhci_irq_msix_unuse(uint32_t nr) "nr %d"
usb_xhci_queue_event(uint32_t vector, uint32_t idx, const char *trb, const char *evt, uint64_t param, uint32_t status, uint32_t control) "v %d, idx %d, %s, %s, p %016" PRIx64 ", s %08x, c 0x%08x"
usb_xhci_fetch_trb(uint64_t addr, const char *name, uint64_t param, uint32_t status, uint32_t control) "addr %016" PRIx64 ", %s, p %016" PRIx64 ", s %08x, c 0x%08x"
usb_xhci_port_reset(uint32_t port, bool warm) "port %d, warm %d"
usb_xhci_port_link(uint32_t port, uint32_t pls) "port %d, pls %d"
usb_xhci_port_notify(uint32_t port, uint32_t pls) "port %d, bits %x"
usb_xhci_slot_enable(uint32_t slotid) "slotid %d"
usb_xhci_slot_disable(uint32_t slotid) "slotid %d"
usb_xhci_slot_address(uint32_t slotid, const char *port) "slotid %d, port %s"
usb_xhci_slot_configure(uint32_t slotid) "slotid %d"
usb_xhci_slot_evaluate(uint32_t slotid) "slotid %d"
usb_xhci_slot_reset(uint32_t slotid) "slotid %d"
usb_xhci_ep_enable(uint32_t slotid, uint32_t epid) "slotid %d, epid %d"
usb_xhci_ep_disable(uint32_t slotid, uint32_t epid) "slotid %d, epid %d"
usb_xhci_ep_set_dequeue(uint32_t slotid, uint32_t epid, uint32_t streamid, uint64_t param) "slotid %d, epid %d, streamid %d, ptr %016" PRIx64
usb_xhci_ep_kick(uint32_t slotid, uint32_t epid, uint32_t streamid) "slotid %d, epid %d, streamid %d"
usb_xhci_ep_stop(uint32_t slotid, uint32_t epid) "slotid %d, epid %d"
usb_xhci_ep_reset(uint32_t slotid, uint32_t epid) "slotid %d, epid %d"
usb_xhci_ep_state(uint32_t slotid, uint32_t epid, const char *os, const char *ns) "slotid %d, epid %d, %s -> %s"
usb_xhci_xfer_start(void *xfer, uint32_t slotid, uint32_t epid, uint32_t streamid) "%p: slotid %d, epid %d, streamid %d"
usb_xhci_xfer_async(void *xfer) "%p"
usb_xhci_xfer_nak(void *xfer) "%p"
usb_xhci_xfer_retry(void *xfer) "%p"
usb_xhci_xfer_success(void *xfer, uint32_t bytes) "%p: len %d"
usb_xhci_xfer_error(void *xfer, uint32_t ret) "%p: ret %d"
usb_xhci_unimplemented(const char *item, int nr) "%s (0x%x)"

# hw/usb/desc.c
usb_desc_device(int addr, int len, int ret) "dev %d query device, len %d, ret %d"
usb_desc_device_qualifier(int addr, int len, int ret) "dev %d query device qualifier, len %d, ret %d"
usb_desc_config(int addr, int index, int len, int ret) "dev %d query config %d, len %d, ret %d"
usb_desc_other_speed_config(int addr, int index, int len, int ret) "dev %d query config %d, len %d, ret %d"
usb_desc_string(int addr, int index, int len, int ret) "dev %d query string %d, len %d, ret %d"
usb_desc_bos(int addr, int len, int ret) "dev %d bos, len %d, ret %d"
usb_desc_msos(int addr, int index, int len, int ret) "dev %d msos, index 0x%x, len %d, ret %d"
usb_set_addr(int addr) "dev %d"
usb_set_config(int addr, int config, int ret) "dev %d, config %d, ret %d"
usb_set_interface(int addr, int iface, int alt, int ret) "dev %d, interface %d, altsetting %d, ret %d"
usb_clear_device_feature(int addr, int feature, int ret) "dev %d, feature %d, ret %d"
usb_set_device_feature(int addr, int feature, int ret) "dev %d, feature %d, ret %d"

# hw/usb/dev-hub.c
usb_hub_reset(int addr) "dev %d"
usb_hub_control(int addr, int request, int value, int index, int length) "dev %d, req 0x%x, value %d, index %d, langth %d"
usb_hub_get_port_status(int addr, int nr, int status, int changed) "dev %d, port %d, status 0x%x, changed 0x%x"
usb_hub_set_port_feature(int addr, int nr, const char *f) "dev %d, port %d, feature %s"
usb_hub_clear_port_feature(int addr, int nr, const char *f) "dev %d, port %d, feature %s"
usb_hub_attach(int addr, int nr) "dev %d, port %d"
usb_hub_detach(int addr, int nr) "dev %d, port %d"
usb_hub_status_report(int addr, int status) "dev %d, status 0x%x"

# hw/usb/dev-uas.c
usb_uas_reset(int addr) "dev %d"
usb_uas_command(int addr, uint16_t tag, int lun, uint32_t lun64_1, uint32_t lun64_2) "dev %d, tag 0x%x, lun %d, lun64 %08x-%08x"
usb_uas_response(int addr, uint16_t tag, uint8_t code) "dev %d, tag 0x%x, code 0x%x"
usb_uas_sense(int addr, uint16_t tag, uint8_t status) "dev %d, tag 0x%x, status 0x%x"
usb_uas_read_ready(int addr, uint16_t tag) "dev %d, tag 0x%x"
usb_uas_write_ready(int addr, uint16_t tag) "dev %d, tag 0x%x"
usb_uas_xfer_data(int addr, uint16_t tag, uint32_t copy, uint32_t uoff, uint32_t usize, uint32_t soff, uint32_t ssize) "dev %d, tag 0x%x, copy %d, usb-pkt %d/%d, scsi-buf %d/%d"
usb_uas_scsi_data(int addr, uint16_t tag, uint32_t bytes) "dev %d, tag 0x%x, bytes %d"
usb_uas_scsi_complete(int addr, uint16_t tag, uint32_t status, uint32_t resid) "dev %d, tag 0x%x, status 0x%x, residue %d"
usb_uas_tmf_abort_task(int addr, uint16_t tag, uint16_t task_tag) "dev %d, tag 0x%x, task-tag 0x%x"
usb_uas_tmf_logical_unit_reset(int addr, uint16_t tag, int lun) "dev %d, tag 0x%x, lun %d"
usb_uas_tmf_unsupported(int addr, uint16_t tag, uint32_t function) "dev %d, tag 0x%x, function 0x%x"

# hw/usb/dev-mtp.c
usb_mtp_reset(int addr) "dev %d"
usb_mtp_command(int dev, uint16_t code, uint32_t trans, uint32_t arg0, uint32_t arg1, uint32_t arg2, uint32_t arg3, uint32_t arg4) "dev %d, code 0x%x, trans 0x%x, args 0x%x, 0x%x, 0x%x, 0x%x, 0x%x"
usb_mtp_success(int dev, uint32_t trans, uint32_t arg0, uint32_t arg1) "dev %d, trans 0x%x, args 0x%x, 0x%x"
usb_mtp_error(int dev, uint16_t code, uint32_t trans, uint32_t arg0, uint32_t arg1) "dev %d, code 0x%x, trans 0x%x, args 0x%x, 0x%x"
usb_mtp_data_in(int dev, uint32_t trans, uint32_t len) "dev %d, trans 0x%x, len %d"
usb_mtp_xfer(int dev, uint32_t ep, uint32_t dlen, uint32_t plen) "dev %d, ep %d, %d/%d"
usb_mtp_nak(int dev, uint32_t ep) "dev %d, ep %d"
usb_mtp_stall(int dev, const char *reason) "dev %d, reason: %s"
usb_mtp_op_get_device_info(int dev) "dev %d"
usb_mtp_op_open_session(int dev) "dev %d"
usb_mtp_op_close_session(int dev) "dev %d"
usb_mtp_op_get_storage_ids(int dev) "dev %d"
usb_mtp_op_get_storage_info(int dev) "dev %d"
usb_mtp_op_get_num_objects(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"
usb_mtp_op_get_object_handles(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"
usb_mtp_op_get_object_info(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"
usb_mtp_op_get_object(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"
usb_mtp_op_get_partial_object(int dev, uint32_t handle, const char *path, uint32_t offset, uint32_t length) "dev %d, handle 0x%x, path %s, off %d, len %d"
usb_mtp_op_unknown(int dev, uint32_t code) "dev %d, command code 0x%x"
usb_mtp_object_alloc(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"
usb_mtp_object_free(int dev, uint32_t handle, const char *path) "dev %d, handle 0x%x, path %s"

# hw/usb/host-libusb.c
usb_host_open_started(int bus, int addr) "dev %d:%d"
usb_host_open_success(int bus, int addr) "dev %d:%d"
usb_host_open_failure(int bus, int addr) "dev %d:%d"
usb_host_close(int bus, int addr) "dev %d:%d"
usb_host_attach_kernel(int bus, int addr, int interface) "dev %d:%d, if %d"
usb_host_detach_kernel(int bus, int addr, int interface) "dev %d:%d, if %d"
usb_host_set_address(int bus, int addr, int config) "dev %d:%d, address %d"
usb_host_set_config(int bus, int addr, int config) "dev %d:%d, config %d"
usb_host_set_interface(int bus, int addr, int interface, int alt) "dev %d:%d, interface %d, alt %d"
usb_host_claim_interface(int bus, int addr, int config, int interface) "dev %d:%d, config %d, if %d"
usb_host_release_interface(int bus, int addr, int interface) "dev %d:%d, if %d"
usb_host_req_control(int bus, int addr, void *p, int req, int value, int index) "dev %d:%d, packet %p, req 0x%x, value %d, index %d"
usb_host_req_data(int bus, int addr, void *p, int in, int ep, int size) "dev %d:%d, packet %p, in %d, ep %d, size %d"
usb_host_req_complete(int bus, int addr, void *p, int status, int length) "dev %d:%d, packet %p, status %d, length %d"
usb_host_req_emulated(int bus, int addr, void *p, int status) "dev %d:%d, packet %p, status %d"
usb_host_req_canceled(int bus, int addr, void *p) "dev %d:%d, packet %p"
usb_host_iso_start(int bus, int addr, int ep) "dev %d:%d, ep %d"
usb_host_iso_stop(int bus, int addr, int ep) "dev %d:%d, ep %d"
usb_host_iso_out_of_bufs(int bus, int addr, int ep) "dev %d:%d, ep %d"
usb_host_reset(int bus, int addr) "dev %d:%d"
usb_host_auto_scan_enabled(void)
usb_host_auto_scan_disabled(void)
usb_host_parse_config(int bus, int addr, int value, int active) "dev %d:%d, value %d, active %d"
usb_host_parse_interface(int bus, int addr, int num, int alt, int active) "dev %d:%d, num %d, alt %d, active %d"
usb_host_parse_endpoint(int bus, int addr, int ep, const char *dir, const char *type, int active) "dev %d:%d, ep %d, %s, %s, active %d"
usb_host_parse_error(int bus, int addr, const char *errmsg) "dev %d:%d, msg %s"

# hw/scsi/scsi-bus.c
scsi_req_alloc(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_req_cancel(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_req_data(int target, int lun, int tag, int len) "target %d lun %d tag %d len %d"
scsi_req_data_canceled(int target, int lun, int tag, int len) "target %d lun %d tag %d len %d"
scsi_req_dequeue(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_req_continue(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_req_continue_canceled(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_req_parsed(int target, int lun, int tag, int cmd, int mode, int xfer) "target %d lun %d tag %d command %d dir %d length %d"
scsi_req_parsed_lba(int target, int lun, int tag, int cmd, uint64_t lba) "target %d lun %d tag %d command %d lba %"PRIu64
scsi_req_parse_bad(int target, int lun, int tag, int cmd) "target %d lun %d tag %d command %d"
scsi_req_build_sense(int target, int lun, int tag, int key, int asc, int ascq) "target %d lun %d tag %d key %#02x asc %#02x ascq %#02x"
scsi_device_set_ua(int target, int lun, int key, int asc, int ascq) "target %d lun %d key %#02x asc %#02x ascq %#02x"
scsi_report_luns(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_inquiry(int target, int lun, int tag, int cdb1, int cdb2) "target %d lun %d tag %d page %#02x/%#02x"
scsi_test_unit_ready(int target, int lun, int tag) "target %d lun %d tag %d"
scsi_request_sense(int target, int lun, int tag) "target %d lun %d tag %d"

# vl.c
vm_state_notify(int running, int reason) "running %d reason %d"
load_file(const char *name, const char *path) "name %s location %s"
runstate_set(int new_state) "new state %d"
system_wakeup_request(int reason) "reason=%d"
qemu_system_shutdown_request(void) ""
qemu_system_powerdown_request(void) ""

# block/qcow2.c
qcow2_writev_start_req(void *co, int64_t sector, int nb_sectors) "co %p sector %" PRIx64 " nb_sectors %d"
qcow2_writev_done_req(void *co, int ret) "co %p ret %d"
qcow2_writev_start_part(void *co) "co %p"
qcow2_writev_done_part(void *co, int cur_nr_sectors) "co %p cur_nr_sectors %d"
qcow2_writev_data(void *co, uint64_t offset) "co %p offset %" PRIx64

# block/qcow2-cluster.c
qcow2_alloc_clusters_offset(void *co, uint64_t offset, int num) "co %p offset %" PRIx64 " num %d"
qcow2_handle_copied(void *co, uint64_t guest_offset, uint64_t host_offset, uint64_t bytes) "co %p guest_offset %" PRIx64 " host_offset %" PRIx64 " bytes %" PRIx64
qcow2_handle_alloc(void *co, uint64_t guest_offset, uint64_t host_offset, uint64_t bytes) "co %p guest_offset %" PRIx64 " host_offset %" PRIx64 " bytes %" PRIx64
qcow2_do_alloc_clusters_offset(void *co, uint64_t guest_offset, uint64_t host_offset, int nb_clusters) "co %p guest_offset %" PRIx64 " host_offset %" PRIx64 " nb_clusters %d"
qcow2_cluster_alloc_phys(void *co) "co %p"
qcow2_cluster_link_l2(void *co, int nb_clusters) "co %p nb_clusters %d"

qcow2_l2_allocate(void *bs, int l1_index) "bs %p l1_index %d"
qcow2_l2_allocate_get_empty(void *bs, int l1_index) "bs %p l1_index %d"
qcow2_l2_allocate_write_l2(void *bs, int l1_index) "bs %p l1_index %d"
qcow2_l2_allocate_write_l1(void *bs, int l1_index) "bs %p l1_index %d"
qcow2_l2_allocate_done(void *bs, int l1_index, int ret) "bs %p l1_index %d ret %d"

# block/qcow2-cache.c
qcow2_cache_get(void *co, int c, uint64_t offset, bool read_from_disk) "co %p is_l2_cache %d offset %" PRIx64 " read_from_disk %d"
qcow2_cache_get_replace_entry(void *co, int c, int i) "co %p is_l2_cache %d index %d"
qcow2_cache_get_read(void *co, int c, int i) "co %p is_l2_cache %d index %d"
qcow2_cache_get_done(void *co, int c, int i) "co %p is_l2_cache %d index %d"
qcow2_cache_flush(void *co, int c) "co %p is_l2_cache %d"
qcow2_cache_entry_flush(void *co, int c, int i) "co %p is_l2_cache %d index %d"

# block/qed-l2-cache.c
qed_alloc_l2_cache_entry(void *l2_cache, void *entry) "l2_cache %p entry %p"
qed_unref_l2_cache_entry(void *entry, int ref) "entry %p ref %d"
qed_find_l2_cache_entry(void *l2_cache, void *entry, uint64_t offset, int ref) "l2_cache %p entry %p offset %"PRIu64" ref %d"

# block/qed-table.c
qed_read_table(void *s, uint64_t offset, void *table) "s %p offset %"PRIu64" table %p"
qed_read_table_cb(void *s, void *table, int ret) "s %p table %p ret %d"
qed_write_table(void *s, uint64_t offset, void *table, unsigned int index, unsigned int n) "s %p offset %"PRIu64" table %p index %u n %u"
qed_write_table_cb(void *s, void *table, int flush, int ret) "s %p table %p flush %d ret %d"

# block/qed.c
qed_need_check_timer_cb(void *s) "s %p"
qed_start_need_check_timer(void *s) "s %p"
qed_cancel_need_check_timer(void *s) "s %p"
qed_aio_complete(void *s, void *acb, int ret) "s %p acb %p ret %d"
qed_aio_setup(void *s, void *acb, int64_t sector_num, int nb_sectors, void *opaque, int flags) "s %p acb %p sector_num %"PRId64" nb_sectors %d opaque %p flags %#x"
qed_aio_next_io(void *s, void *acb, int ret, uint64_t cur_pos) "s %p acb %p ret %d cur_pos %"PRIu64
qed_aio_read_data(void *s, void *acb, int ret, uint64_t offset, size_t len) "s %p acb %p ret %d offset %"PRIu64" len %zu"
qed_aio_write_data(void *s, void *acb, int ret, uint64_t offset, size_t len) "s %p acb %p ret %d offset %"PRIu64" len %zu"
qed_aio_write_prefill(void *s, void *acb, uint64_t start, size_t len, uint64_t offset) "s %p acb %p start %"PRIu64" len %zu offset %"PRIu64
qed_aio_write_postfill(void *s, void *acb, uint64_t start, size_t len, uint64_t offset) "s %p acb %p start %"PRIu64" len %zu offset %"PRIu64
qed_aio_write_main(void *s, void *acb, int ret, uint64_t offset, size_t len) "s %p acb %p ret %d offset %"PRIu64" len %zu"

# hw/display/g364fb.c
g364fb_read(uint64_t addr, uint32_t val) "read addr=0x%"PRIx64": 0x%x"
g364fb_write(uint64_t addr, uint32_t new) "write addr=0x%"PRIx64": 0x%x"

# hw/timer/grlib_gptimer.c
grlib_gptimer_enable(int id, uint32_t count) "timer:%d set count 0x%x and run"
grlib_gptimer_disabled(int id, uint32_t config) "timer:%d Timer disable config 0x%x"
grlib_gptimer_restart(int id, uint32_t reload) "timer:%d reload val: 0x%x"
grlib_gptimer_set_scaler(uint32_t scaler, uint32_t freq) "scaler:0x%x freq: 0x%x"
grlib_gptimer_hit(int id) "timer:%d HIT"
grlib_gptimer_readl(int id, uint64_t addr, uint32_t val) "timer:%d addr 0x%"PRIx64" 0x%x"
grlib_gptimer_writel(int id, uint64_t addr, uint32_t val) "timer:%d addr 0x%"PRIx64" 0x%x"

# hw/intc/grlib_irqmp.c
grlib_irqmp_check_irqs(uint32_t pend, uint32_t force, uint32_t mask, uint32_t lvl1, uint32_t lvl2) "pend:0x%04x force:0x%04x mask:0x%04x lvl1:0x%04x lvl0:0x%04x"
grlib_irqmp_ack(int intno) "interrupt:%d"
grlib_irqmp_set_irq(int irq) "Raise CPU IRQ %d"
grlib_irqmp_readl_unknown(uint64_t addr) "addr 0x%"PRIx64
grlib_irqmp_writel_unknown(uint64_t addr, uint32_t value) "addr 0x%"PRIx64" value 0x%x"

# hw/char/grlib_apbuart.c
grlib_apbuart_event(int event) "event:%d"
grlib_apbuart_writel_unknown(uint64_t addr, uint32_t value) "addr 0x%"PRIx64" value 0x%x"
grlib_apbuart_readl_unknown(uint64_t addr) "addr 0x%"PRIx64""

# hw/sparc/leon3.c
leon3_set_irq(int intno) "Set CPU IRQ %d"
leon3_reset_irq(int intno) "Reset CPU IRQ %d"

# spice-qemu-char.c
spice_vmc_write(ssize_t out, int len) "spice wrottn %zd of requested %d"
spice_vmc_read(int bytes, int len) "spice read %d of requested %d"
spice_vmc_register_interface(void *scd) "spice vmc registered interface %p"
spice_vmc_unregister_interface(void *scd) "spice vmc unregistered interface %p"
spice_vmc_event(int event) "spice vmc event %d"

# hw/intc/lm32_pic.c
lm32_pic_raise_irq(void) "Raise CPU interrupt"
lm32_pic_lower_irq(void) "Lower CPU interrupt"
lm32_pic_interrupt(int irq, int level) "Set IRQ%d %d"
lm32_pic_set_im(uint32_t im) "im 0x%08x"
lm32_pic_set_ip(uint32_t ip) "ip 0x%08x"
lm32_pic_get_im(uint32_t im) "im 0x%08x"
lm32_pic_get_ip(uint32_t ip) "ip 0x%08x"

# hw/char/lm32_juart.c
lm32_juart_get_jtx(uint32_t value) "jtx 0x%08x"
lm32_juart_set_jtx(uint32_t value) "jtx 0x%08x"
lm32_juart_get_jrx(uint32_t value) "jrx 0x%08x"
lm32_juart_set_jrx(uint32_t value) "jrx 0x%08x"

# hw/timer/lm32_timer.c
lm32_timer_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_timer_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_timer_hit(void) "timer hit"
lm32_timer_irq_state(int level) "irq state %d"

# hw/char/lm32_uart.c
lm32_uart_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_uart_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_uart_irq_state(int level) "irq state %d"

# hw/scsi/megasas.c
megasas_init_firmware(uint64_t pa) "pa %" PRIx64 " "
megasas_init_queue(uint64_t queue_pa, int queue_len, uint64_t head, uint64_t tail, uint32_t flags) "queue at %" PRIx64 " len %d head %" PRIx64 " tail %" PRIx64 " flags %x"
megasas_initq_map_failed(int frame) "scmd %d: failed to map queue"
megasas_initq_mapped(uint64_t pa) "queue already mapped at %" PRIx64 ""
megasas_initq_mismatch(int queue_len, int fw_cmds) "queue size %d max fw cmds %d"
megasas_qf_mapped(unsigned int index) "skip mapped frame %x"
megasas_qf_new(unsigned int index, uint64_t frame) "frame %x addr %" PRIx64 ""
megasas_qf_busy(unsigned long pa) "all frames busy for frame %lx"
megasas_qf_enqueue(unsigned int index, unsigned int count, uint64_t context, unsigned int head, unsigned int tail, int busy) "frame %x count %d context %" PRIx64 " head %x tail %x busy %d"
megasas_qf_update(unsigned int head, unsigned int tail, unsigned int busy) "head %x tail %x busy %d"
megasas_qf_map_failed(int cmd, unsigned long frame) "scmd %d: frame %lu"
megasas_qf_complete_noirq(uint64_t context) "context %" PRIx64 " "
megasas_qf_complete(uint64_t context, unsigned int head, unsigned int tail, int busy) "context %" PRIx64 " head %x tail %x busy %d"
megasas_frame_busy(uint64_t addr) "frame %" PRIx64 " busy"
megasas_unhandled_frame_cmd(int cmd, uint8_t frame_cmd) "scmd %d: MFI cmd %x"
megasas_handle_scsi(const char *frame, int bus, int dev, int lun, void *sdev, unsigned long size) "%s dev %x/%x/%x sdev %p xfer %lu"
megasas_scsi_target_not_present(const char *frame, int bus, int dev, int lun) "%s dev %x/%x/%x"
megasas_scsi_invalid_cdb_len(const char *frame, int bus, int dev, int lun, int len) "%s dev %x/%x/%x invalid cdb len %d"
megasas_iov_read_overflow(int cmd, int bytes, int len) "scmd %d: %d/%d bytes"
megasas_iov_write_overflow(int cmd, int bytes, int len) "scmd %d: %d/%d bytes"
megasas_iov_read_underflow(int cmd, int bytes, int len) "scmd %d: %d/%d bytes"
megasas_iov_write_underflow(int cmd, int bytes, int len) "scmd %d: %d/%d bytes"
megasas_scsi_req_alloc_failed(const char *frame, int dev, int lun) "%s dev %x/%x"
megasas_scsi_read_start(int cmd, int len) "scmd %d: transfer %d bytes of data"
megasas_scsi_write_start(int cmd, int len) "scmd %d: transfer %d bytes of data"
megasas_scsi_nodata(int cmd) "scmd %d: no data to be transferred"
megasas_scsi_complete(int cmd, uint32_t status, int len, int xfer) "scmd %d: status %x, len %u/%u"
megasas_command_complete(int cmd, uint32_t status, uint32_t resid) "scmd %d: status %x, residual %d"
megasas_handle_io(int cmd, const char *frame, int dev, int lun, unsigned long lba, unsigned long count) "scmd %d: %s dev %x/%x lba %lx count %lu"
megasas_io_target_not_present(int cmd, const char *frame, int dev, int lun) "scmd %d: %s dev 1/%x/%x LUN not present"
megasas_io_read_start(int cmd, unsigned long lba, unsigned long count, unsigned long len) "scmd %d: start LBA %lx %lu blocks (%lu bytes)"
megasas_io_write_start(int cmd, unsigned long lba, unsigned long count, unsigned long len) "scmd %d: start LBA %lx %lu blocks (%lu bytes)"
megasas_io_complete(int cmd, uint32_t len) "scmd %d: %d bytes"
megasas_iovec_sgl_overflow(int cmd, int index, int limit) "scmd %d: iovec count %d limit %d"
megasas_iovec_sgl_underflow(int cmd, int index) "scmd %d: iovec count %d"
megasas_iovec_sgl_invalid(int cmd, int index, uint64_t pa, uint32_t len) "scmd %d: element %d pa %" PRIx64 " len %u"
megasas_iovec_overflow(int cmd, int len, int limit) "scmd %d: len %d limit %d"
megasas_iovec_underflow(int cmd, int len, int limit) "scmd %d: len %d limit %d"
megasas_handle_dcmd(int cmd, int opcode) "scmd %d: MFI DCMD opcode %x"
megasas_finish_dcmd(int cmd, int size) "scmd %d: MFI DCMD wrote %d bytes"
megasas_dcmd_req_alloc_failed(int cmd, const char *desc) "scmd %d: %s"
megasas_dcmd_internal_submit(int cmd, const char *desc, int dev) "scmd %d: %s to dev %d"
megasas_dcmd_internal_finish(int cmd, int opcode, int lun) "scmd %d: cmd %x lun %d"
megasas_dcmd_internal_invalid(int cmd, int opcode) "scmd %d: DCMD %x"
megasas_dcmd_unhandled(int cmd, int opcode, int len) "scmd %d: opcode %x, len %d"
megasas_dcmd_zero_sge(int cmd) "scmd %d: zero DCMD sge count"
megasas_dcmd_invalid_sge(int cmd, int count) "scmd %d: DCMD sge count %d"
megasas_dcmd_invalid_xfer_len(int cmd, unsigned long size, unsigned long max) "scmd %d: xfer len %ld, max %ld"
megasas_dcmd_enter(int cmd, const char *dcmd, int len) "scmd %d: DCMD %s len %d"
megasas_dcmd_dummy(int cmd, unsigned long size) "scmd %d: xfer len %ld"
megasas_dcmd_set_fw_time(int cmd, unsigned long time) "scmd %d: Set FW time %lx"
megasas_dcmd_pd_get_list(int cmd, int num, int max, int offset) "scmd %d: DCMD PD get list: %d / %d PDs, size %d"
megasas_dcmd_ld_get_list(int cmd, int num, int max) "scmd %d: DCMD LD get list: found %d / %d LDs"
megasas_dcmd_ld_get_info(int cmd, int ld_id) "scmd %d: dev %d"
megasas_dcmd_ld_list_query(int cmd, int flags) "scmd %d: query flags %x"
megasas_dcmd_pd_get_info(int cmd, int pd_id) "scmd %d: dev %d"
megasas_dcmd_pd_list_query(int cmd, int flags) "scmd %d: query flags %x"
megasas_dcmd_reset_ld(int cmd, int target_id) "scmd %d: dev %d"
megasas_dcmd_unsupported(int cmd, unsigned long size) "scmd %d: set properties len %ld"
megasas_abort_frame(int cmd, int abort_cmd) "scmd %d: frame %x"
megasas_abort_no_cmd(int cmd, uint64_t context) "scmd %d: no active command for frame context %" PRIx64 ""
megasas_abort_invalid_context(int cmd, uint64_t context, int abort_cmd) "scmd %d: invalid frame context %" PRIx64 " for abort frame %x"
megasas_reset(int fw_state) "firmware state %x"
megasas_init(int sges, int cmds, const char *mode) "Using %d sges, %d cmds, %s mode"
megasas_msix_raise(int vector) "vector %d"
megasas_msi_raise(int vector) "vector %d"
megasas_irq_lower(void) "INTx"
megasas_irq_raise(void) "INTx"
megasas_intr_enabled(void) "Interrupts enabled"
megasas_intr_disabled(void) "Interrupts disabled"
megasas_msix_enabled(int vector) "vector %d"
megasas_msi_enabled(int vector) "vector %d"
megasas_mmio_readl(const char *reg, uint32_t val) "reg %s: 0x%x"
megasas_mmio_invalid_readl(unsigned long addr) "addr 0x%lx"
megasas_mmio_writel(const char *reg, uint32_t val) "reg %s: 0x%x"
megasas_mmio_invalid_writel(uint32_t addr, uint32_t val) "addr 0x%x: 0x%x"

# hw/audio/milkymist-ac97.c
milkymist_ac97_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_ac97_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_ac97_pulse_irq_crrequest(void) "Pulse IRQ CR request"
milkymist_ac97_pulse_irq_crreply(void) "Pulse IRQ CR reply"
milkymist_ac97_pulse_irq_dmaw(void) "Pulse IRQ DMA write"
milkymist_ac97_pulse_irq_dmar(void) "Pulse IRQ DMA read"
milkymist_ac97_in_cb(int avail, uint32_t remaining) "avail %d remaining %u"
milkymist_ac97_in_cb_transferred(int transferred) "transferred %d"
milkymist_ac97_out_cb(int free, uint32_t remaining) "free %d remaining %u"
milkymist_ac97_out_cb_transferred(int transferred) "transferred %d"

# hw/misc/milkymist-hpdmc.c
milkymist_hpdmc_memory_read(uint32_t addr, uint32_t value) "addr=%08x value=%08x"
milkymist_hpdmc_memory_write(uint32_t addr, uint32_t value) "addr=%08x value=%08x"

# hw/sd/milkymist-memcard.c
milkymist_memcard_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_memcard_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"

# hw/net/milkymist-minimac2.c
milkymist_minimac2_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_minimac2_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_minimac2_mdio_write(uint8_t phy_addr, uint8_t addr, uint16_t value) "phy_addr %02x addr %02x value %04x"
milkymist_minimac2_mdio_read(uint8_t phy_addr, uint8_t addr, uint16_t value) "phy_addr %02x addr %02x value %04x"
milkymist_minimac2_tx_frame(uint32_t length) "length %u"
milkymist_minimac2_rx_frame(const void *buf, uint32_t length) "buf %p length %u"
milkymist_minimac2_rx_transfer(const void *buf, uint32_t length) "buf %p length %d"
milkymist_minimac2_raise_irq_rx(void) "Raise IRQ RX"
milkymist_minimac2_lower_irq_rx(void) "Lower IRQ RX"
milkymist_minimac2_pulse_irq_tx(void) "Pulse IRQ TX"

# hw/misc/milkymist-pfpu.c
milkymist_pfpu_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_pfpu_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_pfpu_vectout(uint32_t a, uint32_t b, uint32_t dma_ptr) "a %08x b %08x dma_ptr %08x"
milkymist_pfpu_pulse_irq(void) "Pulse IRQ"

# hw/input/milkymist-softusb.c
milkymist_softusb_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_softusb_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_softusb_mevt(uint8_t m) "m %d"
milkymist_softusb_kevt(uint8_t m) "m %d"
milkymist_softusb_pulse_irq(void) "Pulse IRQ"

# hw/timer/milkymist-sysctl.c
milkymist_sysctl_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_sysctl_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_sysctl_icap_write(uint32_t value) "value %08x"
milkymist_sysctl_start_timer0(void) "Start timer0"
milkymist_sysctl_stop_timer0(void) "Stop timer0"
milkymist_sysctl_start_timer1(void) "Start timer1"
milkymist_sysctl_stop_timer1(void) "Stop timer1"
milkymist_sysctl_pulse_irq_timer0(void) "Pulse IRQ Timer0"
milkymist_sysctl_pulse_irq_timer1(void) "Pulse IRQ Timer1"

# hw/display/milkymist-tmu2.c
milkymist_tmu2_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_tmu2_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_tmu2_start(void) "Start TMU"
milkymist_tmu2_pulse_irq(void) "Pulse IRQ"

# hw/char/milkymist-uart.c
milkymist_uart_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_uart_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_uart_raise_irq(void) "Raise IRQ"
milkymist_uart_lower_irq(void) "Lower IRQ"

# hw/display/milkymist-vgafb.c
milkymist_vgafb_memory_read(uint32_t addr, uint32_t value) "addr %08x value %08x"
milkymist_vgafb_memory_write(uint32_t addr, uint32_t value) "addr %08x value %08x"

# hw/net/mipsnet.c
mipsnet_send(uint32_t size) "sending len=%u"
mipsnet_receive(uint32_t size) "receiving len=%u"
mipsnet_read(uint64_t addr, uint32_t val) "read addr=0x%" PRIx64 " val=0x%x"
mipsnet_write(uint64_t addr, uint64_t val) "write addr=0x%" PRIx64 " val=0x%" PRIx64 ""
mipsnet_irq(uint32_t isr, uint32_t intctl) "set irq to %d (%02x)"

# hw/isa/pc87312.c
pc87312_io_read(uint32_t addr, uint32_t val) "read addr=%x val=%x"
pc87312_io_write(uint32_t addr, uint32_t val) "write addr=%x val=%x"
pc87312_info_floppy(uint32_t base) "base 0x%x"
pc87312_info_ide(uint32_t base) "base 0x%x"
pc87312_info_parallel(uint32_t base, uint32_t irq) "base 0x%x, irq %u"
pc87312_info_serial(int n, uint32_t base, uint32_t irq) "id=%d, base 0x%x, irq %u"

# hw/scsi/vmw_pvscsi.c
pvscsi_ring_init_data(uint32_t txr_len_log2, uint32_t rxr_len_log2) "TX/RX rings logarithms set to %d/%d"
pvscsi_ring_init_msg(uint32_t len_log2) "MSG ring logarithm set to %d"
pvscsi_ring_flush_cmp(uint64_t filled_cmp_ptr) "new production counter of completion ring is 0x%"PRIx64""
pvscsi_ring_flush_msg(uint64_t filled_cmp_ptr) "new production counter of message ring is 0x%"PRIx64""
pvscsi_update_irq_level(bool raise, uint64_t mask, uint64_t status) "interrupt level set to %d (MASK: 0x%"PRIx64", STATUS: 0x%"PRIx64")"
pvscsi_update_irq_msi(void) "sending MSI notification"
pvscsi_cmp_ring_put(unsigned long addr) "got completion descriptor 0x%lx"
pvscsi_msg_ring_put(unsigned long addr) "got message descriptor 0x%lx"
pvscsi_complete_request(uint64_t context, uint64_t len, uint8_t sense_key) "completion: ctx: 0x%"PRIx64", len: 0x%"PRIx64", sense key: %u"
pvscsi_get_sg_list(int nsg, size_t size) "get SG list: depth: %u, size: %zu"
pvscsi_get_next_sg_elem(uint32_t flags) "unknown flags in SG element (val: 0x%x)"
pvscsi_command_complete_not_found(uint32_t tag) "can't find request for tag 0x%x"
pvscsi_command_complete_data_run(void) "not all data required for command transferred"
pvscsi_command_complete_sense_len(int len) "sense information length is %d bytes"
pvscsi_convert_sglist(uint64_t context, unsigned long addr, uint32_t resid) "element: ctx: 0x%"PRIx64" addr: 0x%lx, len: %ul"
pvscsi_process_req_descr(uint8_t cmd, uint64_t ctx) "SCSI cmd 0x%x, ctx: 0x%"PRIx64""
pvscsi_process_req_descr_unknown_device(void) "command directed to unknown device rejected"
pvscsi_process_req_descr_invalid_dir(void) "command with invalid transfer direction rejected"
pvscsi_process_io(unsigned long addr) "got descriptor 0x%lx"
pvscsi_on_cmd_noimpl(const char* cmd) "unimplemented command %s ignored"
pvscsi_on_cmd_reset_dev(uint32_t tgt, int lun, void* dev) "PVSCSI_CMD_RESET_DEVICE[target %u lun %d (dev 0x%p)]"
pvscsi_on_cmd_arrived(const char* cmd) "command %s arrived"
pvscsi_on_cmd_abort(uint64_t ctx, uint32_t tgt) "command PVSCSI_CMD_ABORT_CMD for ctx 0x%"PRIx64", target %u"
pvscsi_on_cmd_unknown(uint64_t cmd_id) "unknown command %"PRIx64""
pvscsi_on_cmd_unknown_data(uint32_t data) "data for unknown command 0x:%x"
pvscsi_io_write(const char* cmd, uint64_t val) "%s write: %"PRIx64""
pvscsi_io_write_unknown(unsigned long addr, unsigned sz, uint64_t val) "unknown write address: 0x%lx size: %u bytes value: 0x%"PRIx64""
pvscsi_io_read(const char* cmd, uint64_t status) "%s read: 0x%"PRIx64""
pvscsi_io_read_unknown(unsigned long addr, unsigned sz) "unknown read address: 0x%lx size: %u bytes"
pvscsi_init_msi_fail(int res) "failed to initialize MSI, error %d"
pvscsi_state(const char* state) "starting %s ..."
pvscsi_tx_rings_ppn(const char* label, uint64_t ppn) "%s page: %"PRIx64""
pvscsi_tx_rings_num_pages(const char* label, uint32_t num) "Number of %s pages: %u"

# xen-hvm.c
xen_ram_alloc(unsigned long ram_addr, unsigned long size) "requested: %#lx, size %#lx"
xen_client_set_memory(uint64_t start_addr, unsigned long size, bool log_dirty) "%#"PRIx64" size %#lx, log_dirty %i"
xen_ioreq_server_create(uint32_t id) "id: %u"
xen_ioreq_server_destroy(uint32_t id) "id: %u"
xen_ioreq_server_state(uint32_t id, bool enable) "id: %u: enable: %i"
xen_map_mmio_range(uint32_t id, uint64_t start_addr, uint64_t end_addr) "id: %u start: %#"PRIx64" end: %#"PRIx64
xen_unmap_mmio_range(uint32_t id, uint64_t start_addr, uint64_t end_addr) "id: %u start: %#"PRIx64" end: %#"PRIx64
xen_map_portio_range(uint32_t id, uint64_t start_addr, uint64_t end_addr) "id: %u start: %#"PRIx64" end: %#"PRIx64
xen_unmap_portio_range(uint32_t id, uint64_t start_addr, uint64_t end_addr) "id: %u start: %#"PRIx64" end: %#"PRIx64
xen_map_pcidev(uint32_t id, uint8_t bus, uint8_t dev, uint8_t func) "id: %u bdf: %02x.%02x.%02x"
xen_unmap_pcidev(uint32_t id, uint8_t bus, uint8_t dev, uint8_t func) "id: %u bdf: %02x.%02x.%02x"
handle_ioreq(void *req, uint32_t type, uint32_t dir, uint32_t df, uint32_t data_is_ptr, uint64_t addr, uint64_t data, uint32_t count, uint32_t size) "I/O=%p type=%d dir=%d df=%d ptr=%d port=%#"PRIx64" data=%#"PRIx64" count=%d size=%d"
handle_ioreq_read(void *req, uint32_t type, uint32_t df, uint32_t data_is_ptr, uint64_t addr, uint64_t data, uint32_t count, uint32_t size) "I/O=%p read type=%d df=%d ptr=%d port=%#"PRIx64" data=%#"PRIx64" count=%d size=%d"
handle_ioreq_write(void *req, uint32_t type, uint32_t df, uint32_t data_is_ptr, uint64_t addr, uint64_t data, uint32_t count, uint32_t size) "I/O=%p write type=%d df=%d ptr=%d port=%#"PRIx64" data=%#"PRIx64" count=%d size=%d"
cpu_ioreq_pio(void *req, uint32_t dir, uint32_t df, uint32_t data_is_ptr, uint64_t addr, uint64_t data, uint32_t count, uint32_t size) "I/O=%p pio dir=%d df=%d ptr=%d port=%#"PRIx64" data=%#"PRIx64" count=%d size=%d"
cpu_ioreq_pio_read_reg(void *req, uint64_t data, uint64_t addr, uint32_t size) "I/O=%p pio read reg data=%#"PRIx64" port=%#"PRIx64" size=%d"
cpu_ioreq_pio_write_reg(void *req, uint64_t data, uint64_t addr, uint32_t size) "I/O=%p pio write reg data=%#"PRIx64" port=%#"PRIx64" size=%d"
cpu_ioreq_move(void *req, uint32_t dir, uint32_t df, uint32_t data_is_ptr, uint64_t addr, uint64_t data, uint32_t count, uint32_t size) "I/O=%p copy dir=%d df=%d ptr=%d port=%#"PRIx64" data=%#"PRIx64" count=%d size=%d"

# xen-mapcache.c
xen_map_cache(uint64_t phys_addr) "want %#"PRIx64
xen_remap_bucket(uint64_t index) "index %#"PRIx64
xen_map_cache_return(void* ptr) "%p"

# hw/i386/xen/xen_platform.c
xen_platform_log(char *s) "xen platform: %s"

# qemu-coroutine.c
qemu_coroutine_enter(void *from, void *to, void *opaque) "from %p to %p opaque %p"
qemu_coroutine_yield(void *from, void *to) "from %p to %p"
qemu_coroutine_terminate(void *co) "self %p"

# qemu-coroutine-lock.c
qemu_co_queue_run_restart(void *co) "co %p"
qemu_co_queue_next(void *nxt) "next %p"
qemu_co_mutex_lock_entry(void *mutex, void *self) "mutex %p self %p"
qemu_co_mutex_lock_return(void *mutex, void *self) "mutex %p self %p"
qemu_co_mutex_unlock_entry(void *mutex, void *self) "mutex %p self %p"
qemu_co_mutex_unlock_return(void *mutex, void *self) "mutex %p self %p"

# hw/char/escc.c
escc_put_queue(char channel, int b) "channel %c put: 0x%02x"
escc_get_queue(char channel, int val) "channel %c get 0x%02x"
escc_update_irq(int irq) "IRQ = %d"
escc_update_parameters(char channel, int speed, int parity, int data_bits, int stop_bits) "channel %c: speed=%d parity=%c data=%d stop=%d"
escc_mem_writeb_ctrl(char channel, uint32_t reg, uint32_t val) "Write channel %c, reg[%d] = %2.2x"
escc_mem_writeb_data(char channel, uint32_t val) "Write channel %c, ch %d"
escc_mem_readb_ctrl(char channel, uint32_t reg, uint8_t val) "Read channel %c, reg[%d] = %2.2x"
escc_mem_readb_data(char channel, uint32_t ret) "Read channel %c, ch %d"
escc_serial_receive_byte(char channel, int ch) "channel %c put ch %d"
escc_sunkbd_event_in(int ch, const char *name, int down) "QKeyCode 0x%2.2x [%s], down %d"
escc_sunkbd_event_out(int ch) "Translated keycode 0x%2.2x"
escc_kbd_command(int val) "Command %d"
escc_sunmouse_event(int dx, int dy, int buttons_state) "dx=%d dy=%d buttons=%01x"

# hw/scsi/esp.c
esp_error_fifo_overrun(void) "FIFO overrun"
esp_error_unhandled_command(uint32_t val) "unhandled command (%2.2x)"
esp_error_invalid_write(uint32_t val, uint32_t addr) "invalid write of 0x%02x at [0x%x]"
esp_raise_irq(void) "Raise IRQ"
esp_lower_irq(void) "Lower IRQ"
esp_dma_enable(void) "Raise enable"
esp_dma_disable(void) "Lower enable"
esp_get_cmd(uint32_t dmalen, int target) "len %d target %d"
esp_do_busid_cmd(uint8_t busid) "busid 0x%x"
esp_handle_satn_stop(uint32_t cmdlen) "cmdlen %d"
esp_write_response(uint32_t status) "Transfer status (status=%d)"
esp_do_dma(uint32_t cmdlen, uint32_t len) "command len %d + %d"
esp_command_complete(void) "SCSI Command complete"
esp_command_complete_unexpected(void) "SCSI command completed unexpectedly"
esp_command_complete_fail(void) "Command failed"
esp_transfer_data(uint32_t dma_left, int32_t ti_size) "transfer %d/%d"
esp_handle_ti(uint32_t minlen) "Transfer Information len %d"
esp_handle_ti_cmd(uint32_t cmdlen) "command len %d"
esp_mem_readb(uint32_t saddr, uint8_t reg) "reg[%d]: 0x%2.2x"
esp_mem_writeb(uint32_t saddr, uint8_t reg, uint32_t val) "reg[%d]: 0x%2.2x -> 0x%2.2x"
esp_mem_writeb_cmd_nop(uint32_t val) "NOP (%2.2x)"
esp_mem_writeb_cmd_flush(uint32_t val) "Flush FIFO (%2.2x)"
esp_mem_writeb_cmd_reset(uint32_t val) "Chip reset (%2.2x)"
esp_mem_writeb_cmd_bus_reset(uint32_t val) "Bus reset (%2.2x)"
esp_mem_writeb_cmd_iccs(uint32_t val) "Initiator Command Complete Sequence (%2.2x)"
esp_mem_writeb_cmd_msgacc(uint32_t val) "Message Accepted (%2.2x)"
esp_mem_writeb_cmd_pad(uint32_t val) "Transfer padding (%2.2x)"
esp_mem_writeb_cmd_satn(uint32_t val) "Set ATN (%2.2x)"
esp_mem_writeb_cmd_rstatn(uint32_t val) "Reset ATN (%2.2x)"
esp_mem_writeb_cmd_sel(uint32_t val) "Select without ATN (%2.2x)"
esp_mem_writeb_cmd_selatn(uint32_t val) "Select with ATN (%2.2x)"
esp_mem_writeb_cmd_selatns(uint32_t val) "Select with ATN & stop (%2.2x)"
esp_mem_writeb_cmd_ensel(uint32_t val) "Enable selection (%2.2x)"
esp_mem_writeb_cmd_dissel(uint32_t val) "Disable selection (%2.2x)"

# hw/scsi/esp-pci.c
esp_pci_error_invalid_dma_direction(void) "invalid DMA transfer direction"
esp_pci_error_invalid_read(uint32_t reg) "read access outside bounds (reg 0x%x)"
esp_pci_error_invalid_write(uint32_t reg) "write access outside bounds (reg 0x%x)"
esp_pci_error_invalid_write_dma(uint32_t val, uint32_t addr) "invalid write of 0x%02x at [0x%x]"
esp_pci_dma_read(uint32_t saddr, uint32_t reg) "reg[%d]: 0x%8.8x"
esp_pci_dma_write(uint32_t saddr, uint32_t reg, uint32_t val) "reg[%d]: 0x%8.8x -> 0x%8.8x"
esp_pci_dma_idle(uint32_t val) "IDLE (%.8x)"
esp_pci_dma_blast(uint32_t val) "BLAST (%.8x)"
esp_pci_dma_abort(uint32_t val) "ABORT (%.8x)"
esp_pci_dma_start(uint32_t val) "START (%.8x)"
esp_pci_sbac_read(uint32_t reg) "sbac: 0x%8.8x"
esp_pci_sbac_write(uint32_t reg, uint32_t val) "sbac: 0x%8.8x -> 0x%8.8x"

# monitor.c
handle_qmp_command(void *mon, const char *cmd_name) "mon %p cmd_name \"%s\""
monitor_protocol_emitter(void *mon) "mon %p"
monitor_protocol_event_handler(uint32_t event, void *data, uint64_t last, uint64_t now) "event=%d data=%p last=%" PRId64 " now=%" PRId64
monitor_protocol_event_emit(uint32_t event, void *data) "event=%d data=%p"
monitor_protocol_event_queue(uint32_t event, void *data, uint64_t rate, uint64_t last, uint64_t now) "event=%d data=%p rate=%" PRId64 " last=%" PRId64 " now=%" PRId64
monitor_protocol_event_throttle(uint32_t event, uint64_t rate) "event=%d rate=%" PRId64

# hw/net/opencores_eth.c
open_eth_mii_write(unsigned idx, uint16_t v) "MII[%02x] <- %04x"
open_eth_mii_read(unsigned idx, uint16_t v) "MII[%02x] -> %04x"
open_eth_update_irq(uint32_t v) "IRQ <- %x"
open_eth_receive(unsigned len) "RX: len: %u"
open_eth_receive_mcast(unsigned idx, uint32_t h0, uint32_t h1) "MCAST: idx = %u, hash: %08x:%08x"
open_eth_receive_reject(void) "RX: rejected"
open_eth_receive_desc(uint32_t addr, uint32_t len_flags) "RX: %08x, len_flags: %08x"
open_eth_start_xmit(uint32_t addr, unsigned len, unsigned tx_len) "TX: %08x, len: %u, tx_len: %u"
open_eth_reg_read(uint32_t addr, uint32_t v) "MAC[%02x] -> %08x"
open_eth_reg_write(uint32_t addr, uint32_t v) "MAC[%02x] <- %08x"
open_eth_desc_read(uint32_t addr, uint32_t v) "DESC[%04x] -> %08x"
open_eth_desc_write(uint32_t addr, uint32_t v) "DESC[%04x] <- %08x"

# hw/9pfs/virtio-9p.c
v9fs_rerror(uint16_t tag, uint8_t id, int err) "tag %d id %d err %d"
v9fs_version(uint16_t tag, uint8_t id, int32_t msize, char* version) "tag %d id %d msize %d version %s"
v9fs_version_return(uint16_t tag, uint8_t id, int32_t msize, char* version) "tag %d id %d msize %d version %s"
v9fs_attach(uint16_t tag, uint8_t id, int32_t fid, int32_t afid, char* uname, char* aname) "tag %u id %u fid %d afid %d uname %s aname %s"
v9fs_attach_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path) "tag %d id %d type %d version %d path %"PRId64""
v9fs_stat(uint16_t tag, uint8_t id, int32_t fid) "tag %d id %d fid %d"
v9fs_stat_return(uint16_t tag, uint8_t id, int32_t mode, int32_t atime, int32_t mtime, int64_t length) "tag %d id %d stat={mode %d atime %d mtime %d length %"PRId64"}"
v9fs_getattr(uint16_t tag, uint8_t id, int32_t fid, uint64_t request_mask) "tag %d id %d fid %d request_mask %"PRIu64""
v9fs_getattr_return(uint16_t tag, uint8_t id, uint64_t result_mask, uint32_t mode, uint32_t uid, uint32_t gid) "tag %d id %d getattr={result_mask %"PRId64" mode %u uid %u gid %u}"
v9fs_walk(uint16_t tag, uint8_t id, int32_t fid, int32_t newfid, uint16_t nwnames) "tag %d id %d fid %d newfid %d nwnames %d"
v9fs_walk_return(uint16_t tag, uint8_t id, uint16_t nwnames, void* qids) "tag %d id %d nwnames %d qids %p"
v9fs_open(uint16_t tag, uint8_t id, int32_t fid, int32_t mode) "tag %d id %d fid %d mode %d"
v9fs_open_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path, int iounit) "tag %d id %d qid={type %d version %d path %"PRId64"} iounit %d"
v9fs_lcreate(uint16_t tag, uint8_t id, int32_t dfid, int32_t flags, int32_t mode, uint32_t gid) "tag %d id %d dfid %d flags %d mode %d gid %u"
v9fs_lcreate_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path, int32_t iounit) "tag %d id %d qid={type %d version %d path %"PRId64"} iounit %d"
v9fs_fsync(uint16_t tag, uint8_t id, int32_t fid, int datasync) "tag %d id %d fid %d datasync %d"
v9fs_clunk(uint16_t tag, uint8_t id, int32_t fid) "tag %d id %d fid %d"
v9fs_read(uint16_t tag, uint8_t id, int32_t fid, uint64_t off, uint32_t max_count) "tag %d id %d fid %d off %"PRIu64" max_count %u"
v9fs_read_return(uint16_t tag, uint8_t id, int32_t count, ssize_t err) "tag %d id %d count %d err %zd"
v9fs_readdir(uint16_t tag, uint8_t id, int32_t fid, uint64_t offset, uint32_t max_count) "tag %d id %d fid %d offset %"PRIu64" max_count %u"
v9fs_readdir_return(uint16_t tag, uint8_t id, uint32_t count, ssize_t retval) "tag %d id %d count %u retval %zd"
v9fs_write(uint16_t tag, uint8_t id, int32_t fid, uint64_t off, uint32_t count, int cnt) "tag %d id %d fid %d off %"PRIu64" count %u cnt %d"
v9fs_write_return(uint16_t tag, uint8_t id, int32_t total, ssize_t err) "tag %d id %d total %d err %zd"
v9fs_create(uint16_t tag, uint8_t id, int32_t fid, char* name, int32_t perm, int8_t mode) "tag %d id %d fid %d name %s perm %d mode %d"
v9fs_create_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path, int iounit) "tag %d id %d qid={type %d version %d path %"PRId64"} iounit %d"
v9fs_symlink(uint16_t tag, uint8_t id, int32_t fid,  char* name, char* symname, uint32_t gid) "tag %d id %d fid %d name %s symname %s gid %u"
v9fs_symlink_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path) "tag %d id %d qid={type %d version %d path %"PRId64"}"
v9fs_flush(uint16_t tag, uint8_t id, int16_t flush_tag) "tag %d id %d flush_tag %d"
v9fs_link(uint16_t tag, uint8_t id, int32_t dfid, int32_t oldfid, char* name) "tag %d id %d dfid %d oldfid %d name %s"
v9fs_remove(uint16_t tag, uint8_t id, int32_t fid) "tag %d id %d fid %d"
v9fs_wstat(uint16_t tag, uint8_t id, int32_t fid, int32_t mode, int32_t atime, int32_t mtime) "tag %u id %u fid %d stat={mode %d atime %d mtime %d}"
v9fs_mknod(uint16_t tag, uint8_t id, int32_t fid, int mode, int major, int minor) "tag %d id %d fid %d mode %d major %d minor %d"
v9fs_mknod_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path) "tag %d id %d qid={type %d version %d path %"PRId64"}"
v9fs_lock(uint16_t tag, uint8_t id, int32_t fid, uint8_t type, uint64_t start, uint64_t length) "tag %d id %d fid %d type %d start %"PRIu64" length %"PRIu64""
v9fs_lock_return(uint16_t tag, uint8_t id, int8_t status) "tag %d id %d status %d"
v9fs_getlock(uint16_t tag, uint8_t id, int32_t fid, uint8_t type, uint64_t start, uint64_t length)"tag %d id %d fid %d type %d start %"PRIu64" length %"PRIu64""
v9fs_getlock_return(uint16_t tag, uint8_t id, uint8_t type, uint64_t start, uint64_t length, uint32_t proc_id) "tag %d id %d type %d start %"PRIu64" length %"PRIu64" proc_id %u"
v9fs_mkdir(uint16_t tag, uint8_t id, int32_t fid, char* name, int mode, uint32_t gid) "tag %u id %u fid %d name %s mode %d gid %u"
v9fs_mkdir_return(uint16_t tag, uint8_t id, int8_t type, int32_t version, int64_t path, int err) "tag %u id %u qid={type %d version %d path %"PRId64"} err %d"
v9fs_xattrwalk(uint16_t tag, uint8_t id, int32_t fid, int32_t newfid, char* name) "tag %d id %d fid %d newfid %d name %s"
v9fs_xattrwalk_return(uint16_t tag, uint8_t id, int64_t size) "tag %d id %d size %"PRId64""
v9fs_xattrcreate(uint16_t tag, uint8_t id, int32_t fid, char* name, int64_t size, int flags) "tag %d id %d fid %d name %s size %"PRId64" flags %d"
v9fs_readlink(uint16_t tag, uint8_t id, int32_t fid) "tag %d id %d fid %d"
v9fs_readlink_return(uint16_t tag, uint8_t id, char* target) "tag %d id %d name %s"

# target-sparc/mmu_helper.c
mmu_helper_dfault(uint64_t address, uint64_t context, int mmu_idx, uint32_t tl) "DFAULT at %"PRIx64" context %"PRIx64" mmu_idx=%d tl=%d"
mmu_helper_dprot(uint64_t address, uint64_t context, int mmu_idx, uint32_t tl) "DPROT at %"PRIx64" context %"PRIx64" mmu_idx=%d tl=%d"
mmu_helper_dmiss(uint64_t address, uint64_t context) "DMISS at %"PRIx64" context %"PRIx64""
mmu_helper_tfault(uint64_t address, uint64_t context) "TFAULT at %"PRIx64" context %"PRIx64""
mmu_helper_tmiss(uint64_t address, uint64_t context) "TMISS at %"PRIx64" context %"PRIx64""
mmu_helper_get_phys_addr_code(uint32_t tl, int mmu_idx, uint64_t prim_context, uint64_t sec_context, uint64_t address) "tl=%d mmu_idx=%d primary context=%"PRIx64" secondary context=%"PRIx64" address=%"PRIx64""
mmu_helper_get_phys_addr_data(uint32_t tl, int mmu_idx, uint64_t prim_context, uint64_t sec_context, uint64_t address) "tl=%d mmu_idx=%d primary context=%"PRIx64" secondary context=%"PRIx64" address=%"PRIx64""
mmu_helper_mmu_fault(uint64_t address, uint64_t paddr, int mmu_idx, uint32_t tl, uint64_t prim_context, uint64_t sec_context) "Translate at %"PRIx64" -> %"PRIx64", mmu_idx=%d tl=%d primary context=%"PRIx64" secondary context=%"PRIx64""

# target-sparc/int64_helper.c
int_helper_set_softint(uint32_t softint) "new %08x"
int_helper_clear_softint(uint32_t softint) "new %08x"
int_helper_write_softint(uint32_t softint) "new %08x"

# target-sparc/int32_helper.c
int_helper_icache_freeze(void) "Instruction cache: freeze"
int_helper_dcache_freeze(void) "Data cache: freeze"

# target-sparc/win_helper.c
win_helper_gregset_error(uint32_t pstate) "ERROR in get_gregset: active pstate bits=%x"
win_helper_switch_pstate(uint32_t pstate_regs, uint32_t new_pstate_regs) "change_pstate: switching regs old=%x new=%x"
win_helper_no_switch_pstate(uint32_t new_pstate_regs) "change_pstate: regs new=%x (unchanged)"
win_helper_wrpil(uint32_t psrpil, uint32_t new_pil) "old=%x new=%x"
win_helper_done(uint32_t tl) "tl=%d"
win_helper_retry(uint32_t tl) "tl=%d"

# dma-helpers.c
dma_blk_io(void *dbs, void *bs, int64_t sector_num, bool to_dev) "dbs=%p bs=%p sector_num=%" PRId64 " to_dev=%d"
dma_aio_cancel(void *dbs) "dbs=%p"
dma_complete(void *dbs, int ret, void *cb) "dbs=%p ret=%d cb=%p"
dma_blk_cb(void *dbs, int ret) "dbs=%p ret=%d"
dma_map_wait(void *dbs) "dbs=%p"

# ui/console.c
console_gfx_new(void) ""
console_putchar_csi(int esc_param0, int esc_param1, int ch, int nb_esc_params) "escape sequence CSI%d;%d%c, %d parameters"
console_putchar_unhandled(int ch) "unhandled escape character '%c'"
console_txt_new(int w, int h) "%dx%d"
console_select(int nr) "%d"
console_refresh(int interval) "interval %d ms"
displaysurface_create(void *display_surface, int w, int h) "surface=%p, %dx%d"
displaysurface_create_from(void *display_surface, int w, int h, uint32_t format) "surface=%p, %dx%d, format 0x%x"
displaysurface_free(void *display_surface) "surface=%p"
displaychangelistener_register(void *dcl, const char *name) "%p [ %s ]"
displaychangelistener_unregister(void *dcl, const char *name) "%p [ %s ]"
ppm_save(const char *filename, void *display_surface) "%s surface=%p"

# ui/gtk.c
gd_switch(const char *tab, int width, int height) "tab=%s, width=%d, height=%d"
gd_update(const char *tab, int x, int y, int w, int h) "tab=%s, x=%d, y=%d, w=%d, h=%d"
gd_key_event(const char *tab, int gdk_keycode, int qemu_keycode, const char *action) "tab=%s, translated GDK keycode %d to QEMU keycode %d (%s)"
gd_grab(const char *tab, const char *device, bool on) "tab=%s, %s %d"

# ui/vnc.c
vnc_key_guest_leds(bool caps, bool num, bool scroll) "caps %d, num %d, scroll %d"
vnc_key_map_init(const char *layout) "%s"
vnc_key_event_ext(bool down, int sym, int keycode, const char *name) "down %d, sym 0x%x, keycode 0x%x [%s]"
vnc_key_event_map(bool down, int sym, int keycode, const char *name) "down %d, sym 0x%x -> keycode 0x%x [%s]"
vnc_key_sync_numlock(bool on) "%d"
vnc_key_sync_capslock(bool on) "%d"

# ui/input.c
input_event_key_number(int conidx, int number, const char *qcode, bool down) "con %d, key number 0x%x [%s], down %d"
input_event_key_qcode(int conidx, const char *qcode, bool down) "con %d, key qcode %s, down %d"
input_event_btn(int conidx, const char *btn, bool down) "con %d, button %s, down %d"
input_event_rel(int conidx, const char *axis, int value) "con %d, axis %s, value %d"
input_event_abs(int conidx, const char *axis, int value) "con %d, axis %s, value 0x%x"
input_event_sync(void) ""
input_mouse_mode(int absolute) "absolute %d"

# hw/display/vmware_vga.c
vmware_value_read(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_value_write(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_palette_read(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_palette_write(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_scratch_read(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_scratch_write(uint32_t index, uint32_t value) "index %d, value 0x%x"
vmware_setmode(uint32_t w, uint32_t h, uint32_t bpp) "%dx%d @ %d bpp"

# hw/display/virtio-gpu.c
virtio_gpu_cmd_get_display_info(void) ""
virtio_gpu_cmd_get_caps(void) ""
virtio_gpu_cmd_set_scanout(uint32_t id, uint32_t res, uint32_t w, uint32_t h, uint32_t x, uint32_t y) "id %d, res 0x%x, w %d, h %d, x %d, y %d"
virtio_gpu_cmd_res_create_2d(uint32_t res, uint32_t fmt, uint32_t w, uint32_t h) "res 0x%x, fmt 0x%x, w %d, h %d"
virtio_gpu_cmd_res_create_3d(uint32_t res, uint32_t fmt, uint32_t w, uint32_t h, uint32_t d) "res 0x%x, fmt 0x%x, w %d, h %d, d %d"
virtio_gpu_cmd_res_unref(uint32_t res) "res 0x%x"
virtio_gpu_cmd_res_back_attach(uint32_t res) "res 0x%x"
virtio_gpu_cmd_res_back_detach(uint32_t res) "res 0x%x"
virtio_gpu_cmd_res_xfer_toh_2d(uint32_t res) "res 0x%x"
virtio_gpu_cmd_res_flush(uint32_t res, uint32_t w, uint32_t h, uint32_t x, uint32_t y) "res 0x%x, w %d, h %d, x %d, y %d"
virtio_gpu_fence_ctrl(uint64_t fence, uint32_t type) "fence 0x%" PRIx64 ", type 0x%x"
virtio_gpu_fence_resp(uint64_t fence) "fence 0x%" PRIx64

# migration/savevm.c
qemu_loadvm_state_section(unsigned int section_type) "%d"
qemu_loadvm_state_section_partend(uint32_t section_id) "%u"
qemu_loadvm_state_section_startfull(uint32_t section_id, const char *idstr, uint32_t instance_id, uint32_t version_id) "%u(%s) %u %u"
savevm_section_start(const char *id, unsigned int section_id) "%s, section_id %u"
savevm_section_end(const char *id, unsigned int section_id, int ret) "%s, section_id %u -> %d"
savevm_section_skip(const char *id, unsigned int section_id) "%s, section_id %u"
savevm_state_begin(void) ""
savevm_state_header(void) ""
savevm_state_iterate(void) ""
savevm_state_complete(void) ""
savevm_state_cancel(void) ""
vmstate_save(const char *idstr, const char *vmsd_name) "%s, %s"
vmstate_load(const char *idstr, const char *vmsd_name) "%s, %s"
qemu_announce_self_iter(const char *mac) "%s"

# vmstate.c
vmstate_load_field_error(const char *field, int ret) "field \"%s\" load failed, ret = %d"
vmstate_load_state(const char *name, int version_id) "%s v%d"
vmstate_load_state_end(const char *name, const char *reason, int val) "%s %s/%d"
vmstate_load_state_field(const char *name, const char *field) "%s:%s"
vmstate_subsection_load(const char *parent) "%s"
vmstate_subsection_load_bad(const char *parent,  const char *sub) "%s: %s"
vmstate_subsection_load_good(const char *parent) "%s"

# qemu-file.c
qemu_file_fclose(void) ""

# migration/ram.c
migration_bitmap_sync_start(void) ""
migration_bitmap_sync_end(uint64_t dirty_pages) "dirty_pages %" PRIu64""
migration_throttle(void) ""

# hw/display/qxl.c
disable qxl_interface_set_mm_time(int qid, uint32_t mm_time) "%d %d"
disable qxl_io_write_vga(int qid, const char *mode, uint32_t addr, uint32_t val) "%d %s addr=%u val=%u"
qxl_create_guest_primary(int qid, uint32_t width, uint32_t height, uint64_t mem, uint32_t format, uint32_t position) "%d %ux%u mem=%" PRIx64 " %u,%u"
qxl_create_guest_primary_rest(int qid, int32_t stride, uint32_t type, uint32_t flags) "%d %d,%d,%d"
qxl_destroy_primary(int qid) "%d"
qxl_enter_vga_mode(int qid) "%d"
qxl_exit_vga_mode(int qid) "%d"
qxl_hard_reset(int qid, int64_t loadvm) "%d loadvm=%"PRId64""
qxl_interface_async_complete_io(int qid, uint32_t current_async, void *cookie) "%d current=%d cookie=%p"
qxl_interface_attach_worker(int qid) "%d"
qxl_interface_get_init_info(int qid) "%d"
qxl_interface_set_compression_level(int qid, int64_t level) "%d %"PRId64
qxl_interface_update_area_complete(int qid, uint32_t surface_id, uint32_t dirty_left, uint32_t dirty_right, uint32_t dirty_top, uint32_t dirty_bottom) "%d surface=%d [%d,%d,%d,%d]"
qxl_interface_update_area_complete_rest(int qid, uint32_t num_updated_rects) "%d #=%d"
qxl_interface_update_area_complete_overflow(int qid, int max) "%d max=%d"
qxl_interface_update_area_complete_schedule_bh(int qid, uint32_t num_dirty) "%d #dirty=%d"
qxl_io_destroy_primary_ignored(int qid, const char *mode) "%d %s"
qxl_io_log(int qid, const uint8_t *log_buf) "%d %s"
qxl_io_read_unexpected(int qid) "%d"
qxl_io_unexpected_vga_mode(int qid, uint64_t addr, uint64_t val, const char *desc) "%d 0x%"PRIx64"=%"PRIu64" (%s)"
qxl_io_write(int qid, const char *mode, uint64_t addr, const char *aname, uint64_t val, unsigned size, int async) "%d %s addr=%"PRIu64 " (%s) val=%"PRIu64" size=%u async=%d"
qxl_memslot_add_guest(int qid, uint32_t slot_id, uint64_t guest_start, uint64_t guest_end) "%d %u: guest phys 0x%"PRIx64 " - 0x%" PRIx64
qxl_post_load(int qid, const char *mode) "%d %s"
qxl_pre_load(int qid) "%d"
qxl_pre_save(int qid) "%d"
qxl_reset_surfaces(int qid) "%d"
qxl_ring_command_check(int qid, const char *mode) "%d %s"
qxl_ring_command_get(int qid, const char *mode) "%d %s"
qxl_ring_command_req_notification(int qid) "%d"
qxl_ring_cursor_check(int qid, const char *mode) "%d %s"
qxl_ring_cursor_get(int qid, const char *mode) "%d %s"
qxl_ring_cursor_req_notification(int qid) "%d"
qxl_ring_res_push(int qid, const char *mode, uint32_t surface_count, uint32_t free_res, void *last_release, const char *notify) "%d %s s#=%d res#=%d last=%p notify=%s"
qxl_ring_res_push_rest(int qid, uint32_t ring_has, uint32_t ring_size, uint32_t prod, uint32_t cons) "%d ring %d/%d [%d,%d]"
qxl_ring_res_put(int qid, uint32_t free_res) "%d #res=%d"
qxl_set_mode(int qid, int modenr, uint32_t x_res, uint32_t y_res, uint32_t bits, uint64_t devmem) "%d mode=%d [ x=%d y=%d @ bpp=%d devmem=0x%" PRIx64 " ]"
qxl_soft_reset(int qid) "%d"
qxl_spice_destroy_surfaces_complete(int qid) "%d"
qxl_spice_destroy_surfaces(int qid, int async) "%d async=%d"
qxl_spice_destroy_surface_wait_complete(int qid, uint32_t id) "%d sid=%d"
qxl_spice_destroy_surface_wait(int qid, uint32_t id, int async) "%d sid=%d async=%d"
qxl_spice_flush_surfaces_async(int qid, uint32_t surface_count, uint32_t num_free_res) "%d s#=%d, res#=%d"
qxl_spice_monitors_config(int qid) "%d"
qxl_spice_loadvm_commands(int qid, void *ext, uint32_t count) "%d ext=%p count=%d"
qxl_spice_oom(int qid) "%d"
qxl_spice_reset_cursor(int qid) "%d"
qxl_spice_reset_image_cache(int qid) "%d"
qxl_spice_reset_memslots(int qid) "%d"
qxl_spice_update_area(int qid, uint32_t surface_id, uint32_t left, uint32_t right, uint32_t top, uint32_t bottom) "%d sid=%d [%d,%d,%d,%d]"
qxl_spice_update_area_rest(int qid, uint32_t num_dirty_rects, uint32_t clear_dirty_region) "%d #d=%d clear=%d"
qxl_surfaces_dirty(int qid, int surface, int offset, int size) "%d surface=%d offset=%d size=%d"
qxl_send_events(int qid, uint32_t events) "%d %d"
qxl_send_events_vm_stopped(int qid, uint32_t events) "%d %d"
qxl_set_guest_bug(int qid) "%d"
qxl_interrupt_client_monitors_config(int qid, int num_heads, void *heads) "%d %d %p"
qxl_client_monitors_config_unsupported_by_guest(int qid, uint32_t int_mask, void *client_monitors_config) "%d %X %p"
qxl_client_monitors_config_unsupported_by_device(int qid, int revision) "%d revision=%d"
qxl_client_monitors_config_capped(int qid, int requested, int limit) "%d %d %d"
qxl_client_monitors_config_crc(int qid, unsigned size, uint32_t crc32) "%d %u %u"
qxl_set_client_capabilities_unsupported_by_revision(int qid, int revision) "%d revision=%d"

# ui/spice-display.c
qemu_spice_add_memslot(int qid, uint32_t slot_id, unsigned long virt_start, unsigned long virt_end, int async) "%d %u: host virt 0x%lx - 0x%lx async=%d"
qemu_spice_del_memslot(int qid, uint32_t gid, uint32_t slot_id) "%d gid=%u sid=%u"
qemu_spice_create_primary_surface(int qid, uint32_t sid, void *surface, int async) "%d sid=%u surface=%p async=%d"
qemu_spice_destroy_primary_surface(int qid, uint32_t sid, int async) "%d sid=%u async=%d"
qemu_spice_wakeup(uint32_t qid) "%d"
qemu_spice_create_update(uint32_t left, uint32_t right, uint32_t top, uint32_t bottom) "lr %d -> %d,  tb -> %d -> %d"

# hw/display/qxl-render.c
qxl_render_blit(int32_t stride, int32_t left, int32_t right, int32_t top, int32_t bottom) "stride=%d [%d, %d, %d, %d]"
qxl_render_guest_primary_resized(int32_t width, int32_t height, int32_t stride, int32_t bytes_pp, int32_t bits_pp) "%dx%d, stride %d, bpp %d, depth %d"
qxl_render_update_area_done(void *cookie) "%p"

# hw/ppc/spapr_pci.c
spapr_pci_msi(const char *msg, uint32_t ca) "%s (cfg=%x)"
spapr_pci_msi_setup(const char *name, unsigned vector, uint64_t addr) "dev\"%s\" vector %u, addr=%"PRIx64
spapr_pci_rtas_ibm_change_msi(unsigned cfg, unsigned func, unsigned req, unsigned first) "cfgaddr %x func %u, requested %u, first irq %u"
spapr_pci_rtas_ibm_query_interrupt_source_number(unsigned ioa, unsigned intr) "queries for #%u, IRQ%u"
spapr_pci_msi_write(uint64_t addr, uint64_t data, uint32_t dt_irq) "@%"PRIx64"<=%"PRIx64" IRQ %u"
spapr_pci_lsi_set(const char *busname, int pin, uint32_t irq) "%s PIN%d IRQ %u"
spapr_pci_msi_retry(unsigned config_addr, unsigned req_num, unsigned max_irqs) "Guest device at %x asked %u, have only %u"

# hw/pci/pci.c
pci_update_mappings_del(void *d, uint32_t bus, uint32_t func, uint32_t slot, int bar, uint64_t addr, uint64_t size) "d=%p %02x:%02x.%x %d,%#"PRIx64"+%#"PRIx64
pci_update_mappings_add(void *d, uint32_t bus, uint32_t func, uint32_t slot, int bar, uint64_t addr, uint64_t size) "d=%p %02x:%02x.%x %d,%#"PRIx64"+%#"PRIx64

# hw/net/pcnet.c
pcnet_s_reset(void *s) "s=%p"
pcnet_user_int(void *s) "s=%p"
pcnet_isr_change(void *s, uint32_t isr, uint32_t isr_old) "s=%p INTA=%d<=%d"
pcnet_init(void *s, uint64_t init_addr) "s=%p init_addr=%#"PRIx64
pcnet_rlen_tlen(void *s, uint32_t rlen, uint32_t tlen) "s=%p rlen=%d tlen=%d"
pcnet_ss32_rdra_tdra(void *s, uint32_t ss32, uint32_t rdra, uint32_t rcvrl, uint32_t tdra, uint32_t xmtrl) "s=%p ss32=%d rdra=0x%08x[%d] tdra=0x%08x[%d]"

# hw/net/pcnet-pci.c
pcnet_aprom_writeb(void *opaque, uint32_t addr, uint32_t val) "opaque=%p addr=0x%08x val=0x%02x"
pcnet_aprom_readb(void *opaque, uint32_t addr, uint32_t val) "opaque=%p addr=0x%08x val=0x%02x"
pcnet_ioport_read(void *opaque, uint64_t addr, unsigned size) "opaque=%p addr=%#"PRIx64" size=%d"
pcnet_ioport_write(void *opaque, uint64_t addr, uint64_t data, unsigned size) "opaque=%p addr=%#"PRIx64" data=%#"PRIx64" size=%d"
pcnet_mmio_writeb(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"
pcnet_mmio_writew(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"
pcnet_mmio_writel(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"
pcnet_mmio_readb(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"
pcnet_mmio_readw(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"
pcnet_mmio_readl(void *opaque, uint64_t addr, uint32_t val) "opaque=%p addr=%#"PRIx64" val=0x%x"

# hw/intc/xics.c
xics_icp_check_ipi(int server, uint8_t mfrr) "CPU %d can take IPI mfrr=%#x"
xics_icp_accept(uint32_t old_xirr, uint32_t new_xirr) "icp_accept: XIRR %#"PRIx32"->%#"PRIx32
xics_icp_eoi(int server, uint32_t xirr, uint32_t new_xirr) "icp_eoi: server %d given XIRR %#"PRIx32" new XIRR %#"PRIx32
xics_icp_irq(int server, int nr, uint8_t priority) "cpu %d trying to deliver irq %#"PRIx32" priority %#x"
xics_icp_raise(uint32_t xirr, uint8_t pending_priority) "raising IRQ new XIRR=%#x new pending priority=%#x"
xics_set_irq_msi(int srcno, int nr) "set_irq_msi: srcno %d [irq %#x]"
xics_masked_pending(void) "set_irq_msi: masked pending"
xics_set_irq_lsi(int srcno, int nr) "set_irq_lsi: srcno %d [irq %#x]"
xics_ics_write_xive(int nr, int srcno, int server, uint8_t priority) "ics_write_xive: irq %#x [src %d] server %#x prio %#x"
xics_ics_reject(int nr, int srcno) "reject irq %#x [src %d]"
xics_ics_eoi(int nr) "ics_eoi: irq %#x"
xics_alloc(int src, int irq) "source#%d, irq %d"
xics_alloc_failed_hint(int src, int irq) "source#%d, irq %d is already in use"
xics_alloc_failed_no_left(int src) "source#%d, no irq left"
xics_alloc_block(int src, int first, int num, bool lsi, int align) "source#%d, first irq %d, %d irqs, lsi=%d, alignnum %d"
xics_ics_free(int src, int irq, int num) "Source#%d, first irq %d, %d irqs"
xics_ics_free_warn(int src, int irq) "Source#%d, irq %d is already free"

# hw/ppc/spapr.c
spapr_cas_failed(unsigned long n) "DT diff buffer is too small: %ld bytes"
spapr_cas_continue(unsigned long n) "Copy changes to the guest: %ld bytes"

# hw/ppc/spapr_hcall.c
spapr_cas_pvr_try(uint32_t pvr) "%x"
spapr_cas_pvr(uint32_t cur_pvr, bool cpu_match, uint32_t new_pvr, uint64_t pcr) "current=%x, cpu_match=%u, new=%x, compat flags=%"PRIx64

# hw/ppc/spapr_iommu.c
spapr_iommu_put(uint64_t liobn, uint64_t ioba, uint64_t tce, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tce=0x%"PRIx64" ret=%"PRId64
spapr_iommu_get(uint64_t liobn, uint64_t ioba, uint64_t ret, uint64_t tce) "liobn=%"PRIx64" ioba=0x%"PRIx64" ret=%"PRId64" tce=0x%"PRIx64
spapr_iommu_indirect(uint64_t liobn, uint64_t ioba, uint64_t tce, uint64_t iobaN, uint64_t tceN, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tcelist=0x%"PRIx64" iobaN=0x%"PRIx64" tceN=0x%"PRIx64" ret=%"PRId64
spapr_iommu_stuff(uint64_t liobn, uint64_t ioba, uint64_t tce_value, uint64_t npages, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tcevalue=0x%"PRIx64" npages=%"PRId64" ret=%"PRId64
spapr_iommu_pci_put(uint64_t liobn, uint64_t ioba, uint64_t tce, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tce=0x%"PRIx64" ret=%"PRId64
spapr_iommu_pci_get(uint64_t liobn, uint64_t ioba, uint64_t ret, uint64_t tce) "liobn=%"PRIx64" ioba=0x%"PRIx64" ret=%"PRId64" tce=0x%"PRIx64
spapr_iommu_pci_indirect(uint64_t liobn, uint64_t ioba, uint64_t tce, uint64_t iobaN, uint64_t tceN, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tcelist=0x%"PRIx64" iobaN=0x%"PRIx64" tceN=0x%"PRIx64" ret=%"PRId64
spapr_iommu_pci_stuff(uint64_t liobn, uint64_t ioba, uint64_t tce_value, uint64_t npages, uint64_t ret) "liobn=%"PRIx64" ioba=0x%"PRIx64" tcevalue=0x%"PRIx64" npages=%"PRId64" ret=%"PRId64
spapr_iommu_xlate(uint64_t liobn, uint64_t ioba, uint64_t tce, unsigned perm, unsigned pgsize) "liobn=%"PRIx64" 0x%"PRIx64" -> 0x%"PRIx64" perm=%u mask=%x"
spapr_iommu_new_table(uint64_t liobn, void *tcet, void *table, int fd) "liobn=%"PRIx64" tcet=%p table=%p fd=%d"

# hw/ppc/ppc.c
ppc_tb_adjust(uint64_t offs1, uint64_t offs2, int64_t diff, int64_t seconds) "adjusted from 0x%"PRIx64" to 0x%"PRIx64", diff %"PRId64" (%"PRId64"s)"

# util/hbitmap.c
hbitmap_iter_skip_words(const void *hb, void *hbi, uint64_t pos, unsigned long cur) "hb %p hbi %p pos %"PRId64" cur 0x%lx"
hbitmap_reset(void *hb, uint64_t start, uint64_t count, uint64_t sbit, uint64_t ebit) "hb %p items %"PRIu64",%"PRIu64" bits %"PRIu64"..%"PRIu64
hbitmap_set(void *hb, uint64_t start, uint64_t count, uint64_t sbit, uint64_t ebit) "hb %p items %"PRIu64",%"PRIu64" bits %"PRIu64"..%"PRIu64

# target-s390x/ioinst.c
ioinst(const char *insn) "IOINST: %s"
ioinst_sch_id(const char *insn, int cssid, int ssid, int schid) "IOINST: %s (%x.%x.%04x)"
ioinst_chp_id(const char *insn, int cssid, int chpid) "IOINST: %s (%x.%02x)"
ioinst_chsc_cmd(uint16_t cmd, uint16_t len) "IOINST: chsc command %04x, len %04x"

# hw/s390x/css.c
css_enable_facility(const char *facility) "CSS: enable %s"
css_crw(uint8_t rsc, uint8_t erc, uint16_t rsid, const char *chained) "CSS: queueing crw: rsc=%x, erc=%x, rsid=%x %s"
css_chpid_add(uint8_t cssid, uint8_t chpid, uint8_t type) "CSS: add chpid %x.%02x (type %02x)"
css_new_image(uint8_t cssid, const char *default_cssid) "CSS: add css image %02x %s"
css_assign_subch(const char *do_assign, uint8_t cssid, uint8_t ssid, uint16_t schid, uint16_t devno) "CSS: %s %x.%x.%04x (devno %04x)"
css_io_interrupt(int cssid, int ssid, int schid, uint32_t intparm, uint8_t isc, const char *conditional) "CSS: I/O interrupt on sch %x.%x.%04x (intparm %08x, isc %x) %s"
css_adapter_interrupt(uint8_t isc) "CSS: adapter I/O interrupt (isc %x)"

# hw/s390x/virtio-ccw.c
virtio_ccw_interpret_ccw(int cssid, int ssid, int schid, int cmd_code) "VIRTIO-CCW: %x.%x.%04x: interpret command %x"
virtio_ccw_new_device(int cssid, int ssid, int schid, int devno, const char *devno_mode) "VIRTIO-CCW: add subchannel %x.%x.%04x, devno %04x (%s)"

# hw/intc/s390_flic_kvm.c
flic_create_device(int err) "flic: create device failed %d"
flic_no_device_api(int err) "flic: no Device Contral API support %d"
flic_reset_failed(int err) "flic: reset failed %d"

# migration.c
migrate_set_state(int new_state) "new state %d"
migrate_fd_cleanup(void) ""
migrate_fd_error(void) ""
migrate_fd_cancel(void) ""
migrate_pending(uint64_t size, uint64_t max) "pending size %" PRIu64 " max %" PRIu64
migrate_transferred(uint64_t tranferred, uint64_t time_spent, double bandwidth, uint64_t size) "transferred %" PRIu64 " time_spent %" PRIu64 " bandwidth %g max_size %" PRId64
migrate_state_too_big(void) ""
migrate_global_state_post_load(const char *state) "loaded state: %s"
migrate_global_state_pre_save(const char *state) "saved state: %s"

# migration/rdma.c
qemu_rdma_accept_incoming_migration(void) ""
qemu_rdma_accept_incoming_migration_accepted(void) ""
qemu_rdma_accept_pin_state(bool pin) "%d"
qemu_rdma_accept_pin_verbsc(void *verbs) "Verbs context after listen: %p"
qemu_rdma_block_for_wrid_miss(const char *wcompstr, int wcomp, const char *gcompstr, uint64_t req) "A Wanted wrid %s (%d) but got %s (%" PRIu64 ")"
qemu_rdma_block_for_wrid_miss_b(const char *wcompstr, int wcomp, const char *gcompstr, uint64_t req) "B Wanted wrid %s (%d) but got %s (%" PRIu64 ")"
qemu_rdma_cleanup_disconnect(void) ""
qemu_rdma_cleanup_waiting_for_disconnect(void) ""
qemu_rdma_close(void) ""
qemu_rdma_connect_pin_all_requested(void) ""
qemu_rdma_connect_pin_all_outcome(bool pin) "%d"
qemu_rdma_dest_init_trying(const char *host, const char *ip) "%s => %s"
qemu_rdma_dump_gid(const char *who, const char *src, const char *dst) "%s Source GID: %s, Dest GID: %s"
qemu_rdma_exchange_get_response_start(const char *desc) "CONTROL: %s receiving..."
qemu_rdma_exchange_get_response_none(const char *desc, int type) "Surprise: got %s (%d)"
qemu_rdma_exchange_send_issue_callback(void) ""
qemu_rdma_exchange_send_waiting(const char *desc) "Waiting for response %s"
qemu_rdma_exchange_send_received(const char *desc) "Response %s received."
qemu_rdma_fill(int64_t control_len, int size) "RDMA %" PRId64 " of %d bytes already in buffer"
qemu_rdma_init_ram_blocks(int blocks) "Allocated %d local ram block structures"
qemu_rdma_poll_recv(const char *compstr, int64_t comp, int64_t id, int sent) "completion %s #%" PRId64 " received (%" PRId64 ") left %d"
qemu_rdma_poll_write(const char *compstr, int64_t comp, int left, uint64_t block, uint64_t chunk, void *local, void *remote) "completions %s (%" PRId64 ") left %d, block %" PRIu64 ", chunk: %" PRIu64 " %p %p"
qemu_rdma_poll_other(const char *compstr, int64_t comp, int left) "other completion %s (%" PRId64 ") received left %d"
qemu_rdma_post_send_control(const char *desc) "CONTROL: sending %s.."
qemu_rdma_register_and_get_keys(uint64_t len, void *start) "Registering %" PRIu64 " bytes @ %p"
qemu_rdma_registration_handle_compress(int64_t length, int index, int64_t offset) "Zapping zero chunk: %" PRId64 " bytes, index %d, offset %" PRId64
qemu_rdma_registration_handle_finished(void) ""
qemu_rdma_registration_handle_ram_blocks(void) ""
qemu_rdma_registration_handle_ram_blocks_loop(const char *name, uint64_t offset, uint64_t length, void *local_host_addr, unsigned int src_index) "%s: @%" PRIx64 "/%" PRIu64 " host:@%p src_index: %u"
qemu_rdma_registration_handle_register(int requests) "%d requests"
qemu_rdma_registration_handle_register_loop(int req, int index, uint64_t addr, uint64_t chunks) "Registration request (%d): index %d, current_addr %" PRIu64 " chunks: %" PRIu64
qemu_rdma_registration_handle_register_rkey(int rkey) "%x"
qemu_rdma_registration_handle_unregister(int requests) "%d requests"
qemu_rdma_registration_handle_unregister_loop(int count, int index, uint64_t chunk) "Unregistration request (%d): index %d, chunk %" PRIu64
qemu_rdma_registration_handle_unregister_success(uint64_t chunk) "%" PRIu64
qemu_rdma_registration_handle_wait(void) ""
qemu_rdma_registration_start(uint64_t flags) "%" PRIu64
qemu_rdma_registration_stop(uint64_t flags) "%" PRIu64
qemu_rdma_registration_stop_ram(void) ""
qemu_rdma_resolve_host_trying(const char *host, const char *ip) "Trying %s => %s"
qemu_rdma_signal_unregister_append(uint64_t chunk, int pos) "Appending unregister chunk %" PRIu64 " at position %d"
qemu_rdma_signal_unregister_already(uint64_t chunk) "Unregister chunk %" PRIu64 " already in queue"
qemu_rdma_unregister_waiting_inflight(uint64_t chunk) "Cannot unregister inflight chunk: %" PRIu64
qemu_rdma_unregister_waiting_proc(uint64_t chunk, int pos) "Processing unregister for chunk: %" PRIu64 " at position %d"
qemu_rdma_unregister_waiting_send(uint64_t chunk) "Sending unregister for chunk: %" PRIu64
qemu_rdma_unregister_waiting_complete(uint64_t chunk) "Unregister for chunk: %" PRIu64 " complete."
qemu_rdma_write_flush(int sent) "sent total: %d"
qemu_rdma_write_one_block(int count, int block, uint64_t chunk, uint64_t current, uint64_t len, int nb_sent, int nb_chunks) "(%d) Not clobbering: block: %d chunk %" PRIu64 " current %" PRIu64 " len %" PRIu64 " %d %d"
qemu_rdma_write_one_post(uint64_t chunk, long addr, long remote, uint32_t len) "Posting chunk: %" PRIu64 ", addr: %lx remote: %lx, bytes %" PRIu32
qemu_rdma_write_one_queue_full(void) ""
qemu_rdma_write_one_recvregres(int mykey, int theirkey, uint64_t chunk) "Received registration result: my key: %x their key %x, chunk %" PRIu64
qemu_rdma_write_one_sendreg(uint64_t chunk, int len, int index, int64_t offset) "Sending registration request chunk %" PRIu64 " for %d bytes, index: %d, offset: %" PRId64
qemu_rdma_write_one_top(uint64_t chunks, uint64_t size) "Writing %" PRIu64 " chunks, (%" PRIu64 " MB)"
qemu_rdma_write_one_zero(uint64_t chunk, int len, int index, int64_t offset) "Entire chunk is zero, sending compress: %" PRIu64 " for %d bytes, index: %d, offset: %" PRId64
rdma_add_block(const char *block_name, int block, uint64_t addr, uint64_t offset, uint64_t len, uint64_t end, uint64_t bits, int chunks) "Added Block: '%s':%d, addr: %" PRIu64 ", offset: %" PRIu64 " length: %" PRIu64 " end: %" PRIu64 " bits %" PRIu64 " chunks %d"
rdma_block_notification_handle(const char *name, int index) "%s at %d"
rdma_delete_block(void *block, uint64_t addr, uint64_t offset, uint64_t len, uint64_t end, uint64_t bits, int chunks) "Deleted Block: %p, addr: %" PRIu64 ", offset: %" PRIu64 " length: %" PRIu64 " end: %" PRIu64 " bits %" PRIu64 " chunks %d"
rdma_start_incoming_migration(void) ""
rdma_start_incoming_migration_after_dest_init(void) ""
rdma_start_incoming_migration_after_rdma_listen(void) ""
rdma_start_outgoing_migration_after_rdma_connect(void) ""
rdma_start_outgoing_migration_after_rdma_source_init(void) ""

# kvm-all.c
kvm_ioctl(int type, void *arg) "type 0x%x, arg %p"
kvm_vm_ioctl(int type, void *arg) "type 0x%x, arg %p"
kvm_vcpu_ioctl(int cpu_index, int type, void *arg) "cpu_index %d, type 0x%x, arg %p"
kvm_run_exit(int cpu_index, uint32_t reason) "cpu_index %d, reason %d"
kvm_device_ioctl(int fd, int type, void *arg) "dev fd %d, type 0x%x, arg %p"
kvm_failed_reg_get(uint64_t id, const char *msg) "Warning: Unable to retrieve ONEREG %" PRIu64 " from KVM: %s"
kvm_failed_reg_set(uint64_t id, const char *msg) "Warning: Unable to set ONEREG %" PRIu64 " to KVM: %s"

# target-ppc/kvm.c
kvm_failed_spr_set(int str, const char *msg) "Warning: Unable to set SPR %d to KVM: %s"
kvm_failed_spr_get(int str, const char *msg) "Warning: Unable to retrieve SPR %d from KVM: %s"

# TCG related tracing (mostly disabled by default)
# cpu-exec.c
disable exec_tb(void *tb, uintptr_t pc) "tb:%p pc=0x%"PRIxPTR
disable exec_tb_nocache(void *tb, uintptr_t pc) "tb:%p pc=0x%"PRIxPTR
disable exec_tb_exit(void *next_tb, unsigned int flags) "tb:%p flags=%x"

# translate-all.c
translate_block(void *tb, uintptr_t pc, uint8_t *tb_code) "tb:%p, pc:0x%"PRIxPTR", tb_code:%p"

# memory.c
memory_region_ops_read(void *mr, uint64_t addr, uint64_t value, unsigned size) "mr %p addr %#"PRIx64" value %#"PRIx64" size %u"
memory_region_ops_write(void *mr, uint64_t addr, uint64_t value, unsigned size) "mr %p addr %#"PRIx64" value %#"PRIx64" size %u"

# qom/object.c
object_dynamic_cast_assert(const char *type, const char *target, const char *file, int line, const char *func) "%s->%s (%s:%d:%s)"
object_class_dynamic_cast_assert(const char *type, const char *target, const char *file, int line, const char *func) "%s->%s (%s:%d:%s)"

# hw/i386/xen/xen_pvdevice.c
xen_pv_mmio_read(uint64_t addr) "WARNING: read from Xen PV Device MMIO space (address %"PRIx64")"
xen_pv_mmio_write(uint64_t addr) "WARNING: write to Xen PV Device MMIO space (address %"PRIx64")"

# hw/pci/pci_host.c
pci_cfg_read(const char *dev, unsigned devid, unsigned fnid, unsigned offs, unsigned val) "%s %02u:%u @0x%x -> 0x%x"
pci_cfg_write(const char *dev, unsigned devid, unsigned fnid, unsigned offs, unsigned val) "%s %02u:%u @0x%x <- 0x%x"

# hw/vfio/vfio-pci.c
vfio_intx_interrupt(const char *name, char line) " (%s) Pin %c"
vfio_eoi(const char *name) " (%s) EOI"
vfio_enable_intx_kvm(const char *name) " (%s) KVM INTx accel enabled"
vfio_disable_intx_kvm(const char *name) " (%s) KVM INTx accel disabled"
vfio_update_irq(const char *name, int new_irq, int target_irq) " (%s) IRQ moved %d -> %d"
vfio_enable_intx(const char *name) " (%s)"
vfio_disable_intx(const char *name) " (%s)"
vfio_msi_interrupt(const char *name, int index, uint64_t addr, int data) " (%s) vector %d 0x%"PRIx64"/0x%x"
vfio_msix_vector_do_use(const char *name, int index) " (%s) vector %d used"
vfio_msix_vector_release(const char *name, int index) " (%s) vector %d released"
vfio_enable_msix(const char *name) " (%s)"
vfio_enable_msi(const char *name, int nr_vectors) " (%s) Enabled %d MSI vectors"
vfio_disable_msix(const char *name) " (%s)"
vfio_disable_msi(const char *name) " (%s)"
vfio_pci_load_rom(const char *name, unsigned long size, unsigned long offset, unsigned long flags) "Device %s ROM:\n  size: 0x%lx, offset: 0x%lx, flags: 0x%lx"
vfio_rom_read(const char *name, uint64_t addr, int size, uint64_t data) " (%s, 0x%"PRIx64", 0x%x) = 0x%"PRIx64
vfio_pci_size_rom(const char *name, int size) "%s ROM size 0x%x"
vfio_vga_write(uint64_t addr, uint64_t data, int size) " (0x%"PRIx64", 0x%"PRIx64", %d)"
vfio_vga_read(uint64_t addr, int size, uint64_t data) " (0x%"PRIx64", %d) = 0x%"PRIx64
# remove ) =
vfio_generic_window_quirk_read(const char * region_name, const char *name, int index, uint64_t addr, int size, uint64_t data) "%s read(%s:BAR%d+0x%"PRIx64", %d = 0x%"PRIx64
## remove )
vfio_generic_window_quirk_write(const char * region_name, const char *name, int index, uint64_t addr, uint64_t data, int size) "%s write(%s:BAR%d+0x%"PRIx64", 0x%"PRIx64", %d"
# remove ) =
vfio_generic_quirk_read(const char * region_name, const char *name, int index, uint64_t addr, int size, uint64_t data) "%s read(%s:BAR%d+0x%"PRIx64", %d = 0x%"PRIx64
# remove )
vfio_generic_quirk_write(const char * region_name, const char *name, int index, uint64_t addr, uint64_t data, int size) "%s write(%s:BAR%d+0x%"PRIx64", 0x%"PRIx64", %d"
vfio_ati_3c3_quirk_read(uint64_t data) " (0x3c3, 1) = 0x%"PRIx64
vfio_vga_probe_ati_3c3_quirk(const char *name) "Enabled ATI/AMD quirk 0x3c3 BAR4for device %s"
vfio_probe_ati_bar4_window_quirk(const char *name) "Enabled ATI/AMD BAR4 window quirk for device %s"
#issue with )
vfio_rtl8168_window_quirk_read_fake(const char *region_name, const char *name) "%s fake read(%s"
vfio_rtl8168_window_quirk_read_table(const char *region_name, const char *name) "%s MSI-X table read(%s"
vfio_rtl8168_window_quirk_read_direct(const char *region_name, const char *name) "%s direct read(%s"
vfio_rtl8168_window_quirk_write_table(const char *region_name, const char *name) "%s MSI-X table write(%s"
vfio_rtl8168_window_quirk_write_direct(const char *region_name, const char *name) "%s direct write(%s"
vfio_probe_rtl8168_bar2_window_quirk(const char *name) "Enabled RTL8168 BAR2 window quirk for device %s"
vfio_probe_ati_bar2_4000_quirk(const char *name) "Enabled ATI/AMD BAR2 0x4000 quirk for device %s"
vfio_nvidia_3d0_quirk_read(int size, uint64_t data) " (0x3d0, %d) = 0x%"PRIx64
vfio_nvidia_3d0_quirk_write(uint64_t data, int size) " (0x3d0, 0x%"PRIx64", %d)"
vfio_vga_probe_nvidia_3d0_quirk(const char *name) "Enabled NVIDIA VGA 0x3d0 quirk for device %s"
vfio_probe_nvidia_bar5_window_quirk(const char *name) "Enabled NVIDIA BAR5 window quirk for device %s"
vfio_probe_nvidia_bar0_88000_quirk(const char *name) "Enabled NVIDIA BAR0 0x88000 quirk for device %s"
vfio_probe_nvidia_bar0_1800_quirk_id(int id) "Nvidia NV%02x"
vfio_probe_nvidia_bar0_1800_quirk(const char *name) "Enabled NVIDIA BAR0 0x1800 quirk for device %s"
vfio_pci_read_config(const char *name, int addr, int len, int val) " (%s, @0x%x, len=0x%x) %x"
vfio_pci_write_config(const char *name, int addr, int val, int len) " (%s, @0x%x, 0x%x, len=0x%x)"
vfio_setup_msi(const char *name, int pos) "%s PCI MSI CAP @0x%x"
vfio_early_setup_msix(const char *name, int pos, int table_bar, int offset, int entries) "%s PCI MSI-X CAP @0x%x, BAR %d, offset 0x%x, entries %d"
vfio_check_pcie_flr(const char *name) "%s Supports FLR via PCIe cap"
vfio_check_pm_reset(const char *name) "%s Supports PM reset"
vfio_check_af_flr(const char *name) "%s Supports FLR via AF cap"
vfio_pci_hot_reset(const char *name, const char *type) " (%s) %s"
vfio_pci_hot_reset_has_dep_devices(const char *name) "%s: hot reset dependent devices:"
vfio_pci_hot_reset_dep_devices(int domain, int bus, int slot, int function, int group_id) "\t%04x:%02x:%02x.%x group %d"
vfio_pci_hot_reset_result(const char *name, const char *result) "%s hot reset: %s"
vfio_populate_device_region(const char *region_name, int index, unsigned long size, unsigned long offset, unsigned long flags) "Device %s region %d:\n  size: 0x%lx, offset: 0x%lx, flags: 0x%lx"
vfio_populate_device_config(const char *name, unsigned long size, unsigned long offset, unsigned long flags) "Device %s config:\n  size: 0x%lx, offset: 0x%lx, flags: 0x%lx"
vfio_populate_device_get_irq_info_failure(void) "VFIO_DEVICE_GET_IRQ_INFO failure: %m"
vfio_initfn(const char *name, int group_id) " (%s) group %d"
vfio_pci_reset(const char *name) " (%s)"
vfio_pci_reset_flr(const char *name) "%s FLR/VFIO_DEVICE_RESET"
vfio_pci_reset_pm(const char *name) "%s PCI PM Reset"

# hw/vfio/vfio-common.c
vfio_region_write(const char *name, int index, uint64_t addr, uint64_t data, unsigned size) " (%s:region%d+0x%"PRIx64", 0x%"PRIx64 ", %d)"
vfio_region_read(char *name, int index, uint64_t addr, unsigned size, uint64_t data) " (%s:region%d+0x%"PRIx64", %d) = 0x%"PRIx64
vfio_iommu_map_notify(uint64_t iova_start, uint64_t iova_end) "iommu map @ %"PRIx64" - %"PRIx64
vfio_listener_region_add_skip(uint64_t start, uint64_t end) "SKIPPING region_add %"PRIx64" - %"PRIx64
vfio_listener_region_add_iommu(uint64_t start, uint64_t end) "region_add [iommu] %"PRIx64" - %"PRIx64
vfio_listener_region_add_ram(uint64_t iova_start, uint64_t iova_end, void *vaddr) "region_add [ram] %"PRIx64" - %"PRIx64" [%p]"
vfio_listener_region_del_skip(uint64_t start, uint64_t end) "SKIPPING region_del %"PRIx64" - %"PRIx64
vfio_listener_region_del(uint64_t start, uint64_t end) "region_del %"PRIx64" - %"PRIx64
vfio_disconnect_container(int fd) "close container->fd=%d"
vfio_put_group(int fd) "close group->fd=%d"
vfio_get_device(const char * name, unsigned int flags, unsigned int num_regions, unsigned int num_irqs) "Device %s flags: %u, regions: %u, irqs: %u"
vfio_put_base_device(int fd) "close vdev->fd=%d"

# hw/vfio/platform.c
vfio_platform_populate_regions(int region_index, unsigned long flag, unsigned long size, int fd, unsigned long offset) "- region %d flags = 0x%lx, size = 0x%lx, fd= %d, offset = 0x%lx"
vfio_platform_base_device_init(char *name, int groupid) "%s belongs to group #%d"
vfio_platform_realize(char *name, char *compat) "vfio device %s, compat = %s"
vfio_platform_eoi(int pin, int fd) "EOI IRQ pin %d (fd=%d)"
vfio_platform_mmap_set_enabled(bool enabled) "fast path = %d"
vfio_platform_intp_mmap_enable(int pin) "IRQ #%d still active, stay in slow path"
vfio_platform_intp_interrupt(int pin, int fd) "Inject IRQ #%d (fd = %d)"
vfio_platform_intp_inject_pending_lockheld(int pin, int fd) "Inject pending IRQ #%d (fd = %d)"
vfio_platform_populate_interrupts(int pin, int count, int flags) "- IRQ index %d: count %d, flags=0x%x"
vfio_intp_interrupt_set_pending(int index) "irq %d is set PENDING"
vfio_platform_start_irqfd_injection(int index, int fd, int resamplefd) "IRQ index=%d, fd = %d, resamplefd = %d"

#hw/acpi/memory_hotplug.c
mhp_acpi_invalid_slot_selected(uint32_t slot) "0x%"PRIx32
mhp_acpi_ejecting_invalid_slot(uint32_t slot) "0x%"PRIx32
mhp_acpi_read_addr_lo(uint32_t slot, uint32_t addr) "slot[0x%"PRIx32"] addr lo: 0x%"PRIx32
mhp_acpi_read_addr_hi(uint32_t slot, uint32_t addr) "slot[0x%"PRIx32"] addr hi: 0x%"PRIx32
mhp_acpi_read_size_lo(uint32_t slot, uint32_t size) "slot[0x%"PRIx32"] size lo: 0x%"PRIx32
mhp_acpi_read_size_hi(uint32_t slot, uint32_t size) "slot[0x%"PRIx32"] size hi: 0x%"PRIx32
mhp_acpi_read_pxm(uint32_t slot, uint32_t pxm) "slot[0x%"PRIx32"] proximity: 0x%"PRIx32
mhp_acpi_read_flags(uint32_t slot, uint32_t flags) "slot[0x%"PRIx32"] flags: 0x%"PRIx32
mhp_acpi_write_slot(uint32_t slot) "set active slot: 0x%"PRIx32
mhp_acpi_write_ost_ev(uint32_t slot, uint32_t ev) "slot[0x%"PRIx32"] OST EVENT: 0x%"PRIx32
mhp_acpi_write_ost_status(uint32_t slot, uint32_t st) "slot[0x%"PRIx32"] OST STATUS: 0x%"PRIx32
mhp_acpi_clear_insert_evt(uint32_t slot) "slot[0x%"PRIx32"] clear insert event"
mhp_acpi_clear_remove_evt(uint32_t slot) "slot[0x%"PRIx32"] clear remove event"
mhp_acpi_pc_dimm_deleted(uint32_t slot) "slot[0x%"PRIx32"] pc-dimm deleted"
mhp_acpi_pc_dimm_delete_failed(uint32_t slot) "slot[0x%"PRIx32"] pc-dimm delete failed"

# hw/i386/pc.c
mhp_pc_dimm_assigned_slot(int slot) "0x%d"
mhp_pc_dimm_assigned_address(uint64_t addr) "0x%"PRIx64

# target-s390x/kvm.c
kvm_enable_cmma(int rc) "CMMA: enabling with result code %d"
kvm_clear_cmma(int rc) "CMMA: clearing with result code %d"
kvm_failed_cpu_state_set(int cpu_index, uint8_t state, const char *msg) "Warning: Unable to set cpu %d state %" PRIu8 " to KVM: %s"
kvm_sigp_finished(uint8_t order, int cpu_index, int dst_index, int cc) "SIGP: Finished order %u on cpu %d -> cpu %d with cc=%d"

# hw/dma/i8257.c
i8257_unregistered_dma(int nchan, int dma_pos, int dma_len) "unregistered DMA channel used nchan=%d dma_pos=%d dma_len=%d"

# target-s390x/cpu.c
cpu_set_state(int cpu_index, uint8_t state) "setting cpu %d state to %" PRIu8
cpu_halt(int cpu_index) "halting cpu %d"
cpu_unhalt(int cpu_index) "unhalting cpu %d"

# hw/arm/virt-acpi-build.c
virt_acpi_setup(void) "No fw cfg or ACPI disabled. Bailing out."

# audio/alsaaudio.c
alsa_revents(int revents) "revents = %d"
alsa_pollout(int i, int fd) "i = %d fd = %d"
alsa_set_handler(int events, int index, int fd, int err) "events=%#x index=%d fd=%d err=%d"
alsa_wrote_zero(int len) "Failed to write %d frames (wrote zero)"
alsa_read_zero(long len) "Failed to read %ld frames (read zero)"
alsa_xrun_out(void) "Recovering from playback xrun"
alsa_xrun_in(void) "Recovering from capture xrun"
alsa_resume_out(void) "Resuming suspended output stream"
alsa_resume_in(void) "Resuming suspended input stream"
alsa_no_frames(int state) "No frames available and ALSA state is %d"

# audio/ossaudio.c
oss_version(int version) "OSS version = %#x"
oss_invalid_available_size(int size, int bufsize) "Invalid available size, size=%d bufsize=%d"
