# WHID's Pinouts #

## P1 Atmega 32u4 Pinouts

SPI pins for ATMega32U4. You can re-flash 32U4 through these pins.

<img src="https://raw.githubusercontent.com/whid-injector/WHID/master/tools/hardware/p1-atmega-pinout.png" width="300">

## P2 USB Pinouts

The pin closer to USB-A is GND. The pins are:

* GND 
* D+ 
* D-  
* VCC 

<img src="https://raw.githubusercontent.com/whid-injector/WHID/master/tools/hardware/p2-usb-pinout.png" width="300">

## LED

The LED wire to D11. It can be controled by ATMega32U4. 