## clock_reply_server

Function - Handle kernel-generated alarm.

### SYNOPSIS

    boolean_t	clock_reply_server
    		(mach_msg_header_t	request_msg,
    		mach_msg_header_t	reply_ms);

### PARAMETERS

in_msg
  [pointer to in structure] The alarm message received from the kernel.

out_msg
  [out structure] Not used.

### DESCRIPTION

The clock_reply_server function is the MIG generated server handling function to handle messages from the kernel corresponding to clock alarms. Such messages are delivered to the alarm reply port named in a clock_alarm call. The clock_reply_server function performs all necessary argument handling for this kernel message and calls the appropriate handling function. These functions must be supplied by the caller.

### RETURN VALUES

TRUE
  The message was handled and the appropriate function was called.

FALSE
  The message did not apply to the alarm mechanism and no other action was taken.

### RELATED INFORMATION

Functions: clock_alarm_reply.